CD 2600 H v51

# Parameters

-     Serial number

-     Administrator password

-     Data type identifier

-     Object Identifier/ Installation addresss

-     [EtYP] - Operation mode of electronic cassette

-     [ EAu ] - Sound signal of sign selected from the keyboard

-     [ ton  ] - Multitone signalling of sign selected from the keyboard

-     [  dJ   ] - dJ

-     [ tOc  ] - Waiting time for picking up the receiver in seconds

-     [  tro  ] - Time of conversation

-     [ t1d  ] - Time of signal generation

-     [ tPA  ] - Pause time

-     [  trY  ] - Time of electrocatch operation in second

-     [ FrY  ] -Frequency of electro-catch supply voltage in Hz

-     [ APo ] - Acoustic confirming opening the electrocatch

-     [ CEn ] - Switching on coded lock service

-     [  idE  ] - Switching on/off electronic keys

-     [  idA  ] -  Registration of electronic keys by users

-     [ NbL  ] - Mode with building numbering

-     [ LdP  ] -  Directing of not serviced numbers

-     [ NbP  ] - Block number for directing of not serviced numbers

# Electronic keys

-     Addition electronic key

-     Verification electronic key

-     Deleting electronic key

# Divided by subject

-     Numbering modes

-     Code of coded lock

-     Supply of camera and illumination

-     Electro-catch

-     Calling options

-     Electronic keys

## Serial number

A unique serial number of the processor, according to which computes an array of electronics in the cassette lock codes. It is printed on a sticker on the processor.
You can edit it, which is useful for example in the case of edition operation mode of electronic cassette from U to H. It can take values from 0000 to 9999. If in the number is the digit 0, then it must also be entered.
Parameter changes can be made insection [ System parameters – grouped by functionality ].

top of page

## Administrator password

Default administrator password is the serial number printed on a sticker on the processor.
You can edit it in the ISD-02 program. It can take values from 0000 to 9999. If in the the number is the digit 0, then it must also be entered.
NOTE!
If you forget password, then without interface ISD-02 and ISD-02 program it is impossible to retrieve it and it will be necessary to restore the default settings electronic cassette, which involves the loss of all entered settings.
Administrator password can be changed in section [ System parameters – grouped by functionality ].

top of page

## Data type identifier

Since version 6.7 software of electronic cassette in EEPROM memory is saved a special identifier that identifies system type, software version and operation mode of electronic cassette ( U or H ). Data type identifier allow self identification of electronic cassette type during receiving data from the EEPROM memory to ISD-02 program.
NOTE!
During each process of receiving data from the EEPROM memory of it should be noted that the program correctly determined the electronic cassette type. In the case of an erroneous reading, set the parameter [Data type identifier] yourself.

Data type identifier is composed of:

- first digit define operation mode of electronic cassette
  - 0 - subordinate entrance ( U ),
  - 1 – main entrance ( H ),
- next two digits identify the type of system
  - 52 – system CD-2502
  - 31 – system CD-3100
- last two digits indicate the version of the software –e.g. 65, 66, itp.

top of page

## Object Identifier/ Installation addresss

addresss or name of the object, in which the electronic cassette is installed. Parameter help more easily identify the data and the files.
Name can contain 20 characters.
During saving data into files it will be default name of file -e.g.

3100_H70_1234_Dabrowskiego 249.bin
To change value [ Object Identifier/ Installation address] in section [ System parameters – grouped by functionality ].

top of page

## [EtYP] - Operation mode of electronic cassette

Parameter defining operation mode of electronic cassette:

- 0 - subordinate entrance - U
- 1 - main entrance - H

In a system with entrance hierarchy there are two types of entrances: the main entrance and subordinate entrances. System CD-2502 can operate for one main entrance and max. 64 subordinate entrances. From the main entrance a connection can be made with each apartment in any building or staircase serviced by the entry phone system. Using panels at the entrance to staircase (subordinate entrance) a connection can be made with the apartments located in this staircase only. Entry phones at subordinate entrances can be used independently. Default setting of the cassette is configured to operate with the subordinate entrance (U).

NOTE!
The parameter is not editable! To change the mode cassette electronics - see Menu/Instruction section Changing the Operation mode of electronic cassette.

top of page

## [ EAu] - Sound signal of sign selected from the keyboard

If this parameter is [ On ], then selection of any sign from the keyboard may be signalized with short acoustic signals heard on the speaker panel.

top of page

## [ ton] - Multitone signalling of sign selected from the keyboard

If this parameter is [ Off ], then selection of a key may be signalled with the same sound (one tone signalling) or (if [ ton ]=[ On ]) for every key sound of different pitch may be attributed (multitone signalling). The use of this function requires fulfilling the following condition [ EAu ]=1 and [ ton ]=1.

top of page

## [ dJ] - dJ

Duration of acoustic signal which signals selection of any sign from the keyboard is as long as time of keystroke but no longer then 1 second.
The use of this function requires fulfilling the following condition [ EAu ] and [ ton ].
Parameter was add in version 6.6 software of electronic cassette.

top of page

## [ trY] - Time of electro-catch operation in second [s]

Time of electrocatch operation in second [s].

top of page

## [ FrY] - Frequency of electro-catch supply voltage [Hz]

Electro-catch supplied with alternating voltage from a transformer makes a characteristic sound (humming) which is often associated with opening of door. This parameter makes it possible to simulate the operation of an electro-catch.
Entering value [ 0 ] makes that an electro-catch will operate without making any sound.
NOTE!
Electromagnetic lock should be supplied by voltage 12 V DC/1A.[ FrY] = [ 0 ]!

top of page

## [ APo ] - Acoustic confirming opening the electrocatch

If parameter [ APo ] in section [ System parameters – grouped by functionality → Door opening parameters ] or [ Parameters – order according to the system → Numerical parameters ] is set up on value [ 1 ] each opening of electro-catch will be signalized in external panel by acoustic signal.

top of page

## [ CEn] - Switching on coded lock service

Setting parameter [ CEn ] to [ Off ] value makes that function of coded lock will be switched off for all users regardless of setting for the individual apartments.
If parameter is set to [ On ] is possible switched off that function for indywidual users in section [ Lock codes / Locks Options ] setting parameter [ Lock code ] to "[-] - Off".

top of page

## [ idE] - Switching on/off electronic keys

In section [ System parameters – grouped by functionality → Code lock parameters] or [ Parameters – order according to the system → Bit Parameters ] default value parameter [ idE ] is [ On ] - function of coded lock is switched on for all users.

top of page

## [ idA] - Registration of electronic keys by users

In a system is possible registration of electronic keys by users. Setting parameter [ idA ] value to [ On ] in section [ System parameters – grouped by functionality → Code lock parameters] or [ Parameters – order according to the system → Bit Parameters ] permits users to register new electronic keys from user's menu.

top of page

## [NbL ] - Mode with building numbering

Switches on the mode with the building numbering. This numbering mode can be used only in entry phone system with entrance hierarchy (main entrance and subordinate entrances). This numbering mode allows repeating apartment numbers in different buildings.
In electronic cassette for subordinate entrance set parameter [ nbL ] (block number) to value higher then zero.
The operation should be repeated for other staircases (buildings). Values [ nbL ] can be repeated in subordinate systems provided that these systems operate with other logical numbers of uniphones.
In order to get connection with an apartment from an external panel at the main entrance one should first of all select building number and then apartment number.

top of page

## [ LdP ] - Directing of not serviced numbers

The value parameter indicates the logic number to which all numbers which are not serviced will be directed.
All numbers which are not serviced by entry phone CD-2502, will be directed to uniphone number given as LdP value, connected to electronic cassette which parameter nbL is the same as parameter NbP. If local number is in the range of serviced number ( parameters [ LLo ] and [ LHi ]) and it is [Off] (parameter [ Mode ]in section [ Lock codes / Locks Options ] is set to "[-] - Off") in subordinate entrance (U), than dial the uniphone which is switched off will cause the call forward.

top of page

## [ NbP ] - Block number for directing of not serviced numbers

All numbers which are not serviced by entry phone CD-2502, will be directed to uniphone number given as [ LdP ] value, connected to electronic cassette which parameter [ nbL ] is the same as parameter [ NbP ] Set parameter [ NbP ] in section [ System parameters – grouped by functionality → Flats Numeration ] or [ Parameters – order according to the system → Numerical parameters ].

top of page

# Divided by subject

## Numbering modes

Digital entry phone as a standard can operate numbers within a range 1...255 (Normal mode), however, very often it is necessary to operate higher numbers or numbers of considerably wider range. This is possible owing to different numbering modes:

- Numbering mode with range shift
- Hotel numbering mode
- Mode with building numbering

### Physical number

Number of uniphone (programmed by jumpers) within a range 1...255.

### Logical number

Number under which a uniphone rings after having selected the number from the keyboard - within a range 1...9998.

### Normal mode

In normal mode physical number of uniphone (programmed by jumpers) corresponds to logical number (selected from the keyboard of talking cassette). This is a default mode of operation of entry phone exchange.

### Mode with building numbering

This numbering mode can be used only in entry phone system with entrance hierarchy. This numbering mode allows repeating apartment numbers in different buildings.
In order to get connection with an apartment from an external panel at the main entrance one should first of all select building number and then apartment number.
In electronic cassette for subordinate entrance set parameter [ nbL ] (block number) to value higher then zero and in electronic cassette for main entrance parameter [ NbL ] to value [ On ].
Values [ nbL ] can be repeated in subordinate systems provided that these systems operate with other logical numbers of uniphones.

### Directing of not serviced numbers

All numbers which are not serviced by entry phone CD-2502, will be directed to uniphone number given as [ LdP ] value, connected to electronic cassette which parameter [ nbL ] is the same as parameter [ NbP ].
*Since version 6.7 software of electronic cassette - If local number is in the range of serviced numbers and is turn off, than is automatically treated as unserviced number (parameter [ Mode ] in section [ Lock codes / Locks Options] in subordinate entrance

top of page

## Code of coded lock

To each apartment one four digital number is attributed which is preliminary defined in the entry phone production process.
To activate this function set parameter [ CEn ] to [ On ]. Function of coded lock will be switched on for all users regardless of setting for the individual apartments.
Code of coded lock can be changed by installing specialist or user (if parameter [ CEd ] is set to [ On ]).
Code of coded lock are declared only in the subordinate entrance cassette (U).

top of page

## Supply of camera and illumination

### Normal mode

Supply of camera and illumination of camera in external panel is turn on only during the conversation. Users can not monitor picture from camera.This is default mode - parameter [ CAon ] in section [ System parameters – grouped by functionality → Operation parameters of the system ] or [ Parameters – order according to the system → Bit Parameters ] has value [ OFF ]. If users want to monitor picture from camera continuously [ CAon ] should be set to [ On ].

### Continuously mode

Supply of camera and illumination of camera in external panel is continuously. If users want to monitor picture from camera also in the night, than the illumination of camera should be turn on continuously. In section [ System parameters – grouped by functionality → Video signal service options ] or [ Parameters – order according to the system → Bit Parameters ] parameter [ CAon ] should be set to [ On ].
NOTE! Even if illumination of camera is turn on continuously, it will be turn off automatically by photoelement in case of good enough external illumination.

top of page

## Door opening parameters

### Time of electro-catch operation in second [s]

Time of electrocatch operation [ trY ] can be set in section [ System parameters – grouped by functionality → Door opening parameters ] or [ Parameters – order according to the system → Numerical parameters ].

### Frequency of electro-catch supply voltage [Hz]

Entering value [ 0 ] to parameter [ FrY ] in section [ System parameters – grouped by functionality → Door opening parameters ] or [ Parameters – order according to the system → Numerical parameters ] makes that an electro-catch will operate without making any sound.
Entering value diffrent then [ 0 ] makes a characteristic sound (humming) which is often associated with opening of door.
Since version 6.7 software of electronic cassette - first 250ms always DC. NOTE!
Electromagnetic lock should be supplied by voltage 12 V DC/1A.[ FrY] = [ 0 ]!

top of page

## Calling options

Calling signal consists of several parts:

- Calling signal – multiplicity of parameters:
  - Time of individual tone generation [ t1t ] - consists of three tones of different frequency F0 (1 kHz), F1 and F2
  - Time of signal generation [ t1d ]
  - Pause time between successive signals ( if number of bells are set to more then 1) [ tPA ]
  and
- Waiting time for picking up the receiver [ tOC ]

Parameters: number of bells, calling ton, calling volume can be set for indywidual users. Signal frequency, time of individual tone generation, pause time, waiting time for picking up the receiver are global parameters for all users conected to this electronic cassette.

Successive tons of different frequency [ F0 ] (1 kHz), [ F1 ] and [ F2 ] form single signal [ t1d ].

### [ t1d ]

Time of signal generation [*10ms] consists of signals [ t1t ] of different frequency.

### [ tPA ]

Pause time *10[ms] after signal [ t1d ]

### [ tOc ]

Waiting time for picking up the receiver in seconds

top of page

## Electronic keys

Entry phone CD-2502 can be equipped with electronic key reader. There are three kinds of keys in entry phone:

- service keys enable change of entry phone configuration,
- special keys are used by postmen, administration etc.
- keys for the occupants.

Keys should be registered at both the main and subordinate entrance. At the main entrance keys attributed to apartment cannot be registered. Entry phone users can register their own electronic keys. This possibility can be switched on globally by setting parameter [ idA] to value [ On ].

- Switching on electronic key
  Default value parameter [ idE] is [ On ] - users can register their own electronic keys. In another case, parameter [ idE] should be changed in main and subordinate entrance electronic cassette.
- Registration of electronic keys by users
  In a system is possible registration of electronic keys by users. Setting parameter [ idA ] value to [ On ]

### Addition

ISD-02 interface allow registration electronic keys in electronic cassette, addition of keys with attributing to apartment, addition on the selected item in memory, and copying keys ( all or whole section) from one electronic cassette to other, or saving settings in file. Using program ISD-02 it is possible to write and read data to the table to / from a file with the extension *.tm, that is so after programmed keys in one electronic cassette it is easily to copy it to another located in the system (for example, to copy from subordinate entrance cassette tapes to main entrance cassette). To save the table select in section [ Electronic keys ] the area you want to copy and press the right mouse button and choose [ Save to file ], and give it a name. To load data into an table, press the right mouse button in the line of the table and choose [ Import from file ].
NOTE!The data that we import from the file will be inserted into the cell line which pointed out. Data in the table will be replaced data imported from the file.
Example:
In file is 12 keys, if we paste them from position 100 then data from positions 100-111 will be deleted and replaced by new. Saved file can be edited. To make change it should be opened in any program to text edition (eg. notepad) made data changes, and finally file must be saved
Besides addition keys by installing specialist it is possible addition keys by users after setting parameter [ idA] to [ On ].

The program allows addition:

#### One electronic key

If you want to add one electronic key, then in section [ Electronic keys ] choose [ Add ] and apply key to the reader ISD. The serial number of electronic key will bereading and show in the box [Serial Number]. This key will be add to first free position. If this key was earlier registrated it will not be add – line with this particular key will be highlighted.

#### Several keys at once

If you want to add several keys at once, then choose [ Add ] and apply all keys successively to the reader ISD. They will be successively added to the first free position.

#### Addition to Position

If you want to add one electronic key tospecific position, then in section [ Electronic keys ]:

- select the position of the cursor,
- choose [ Add to Position ]
- apply key to the reader ISD.

### Verification

#### Verification the key is already registered in the system

If you want to verify that the key is already registered in the system - in section [ Electronic keys ] choose [ Verify key ] and apply key to the reader ISD. If this key was earlier registrated line with this particular key will be highlighted.

### Registering one key in several electronic cassettes

There is possibility of addition one key to several electronic cassette (eg. several subordinate entrances and one main entrance, or only to subordinate entrances). For postmen, administration etc. aside an area designated numbers 1000-1019, which can select and save the file, and during programming other electronic cassette import selected area table to area designed for special keys used by postmen, administration etc. in section [ Electronic keys ].

### Deleting key

Deleting the key from memory will take place after marking line with key and pressing on the keyboard 'Delete'. Deleting all keys from memory will take place after marking any cell in the table and pressing at the same time 'ctrl' and 'a'on the keyboard and next 'Delete'.

top of page

###### v1.0 (24-11-2010)