CD 2600 U v53x

# Parameters

-     Serial number

-     Administrator password

-     Data type identifier

-     Object Identifier/ Installation addresss

-     [EtYP] - Operation mode of electronic cassette

-     [ EAu ] - Sound signal of sign selected from the keyboard

-     [ ton  ] - Multitone signalling of sign selected from the keyboard

-     [  dJ   ] - dJ

-     [ CAon ] - Supply of camera and illumination

-     [ CAin ] - Supported video inputs

-     [ CAtP ] - Switching picture time interval [s]

-     [ 3C   ] - Switching on three-position display

-     [ tOc  ] - Waiting time for picking up the receiver

-     [  tro  ] - Time of conversation

-     [ t1d  ] - Time of signal generation

-     [ tPA  ] - Pause time

-     [  trY  ] - Time of electrocatch operation

-     [ FrY  ] - Frequency of electro-catch supply voltage [Hz]

-     [ APo ] - Acoustic confirming opening the electrocatch

-     [ Ent  ] - 'Fast entrance'

-     [ CEn ] - Switching on coded lock service

-     [ CEd ] - Permission to edition of coded lock codes by occupants>

-     [ CPo ] - Permission to confirm the use of lock code

-     [ CEr  ] - Confirming the use of a wrong code of coded lock

-     [ CHA ] - Request to enter code of coded lock during entering user's menu

-     [  idE  ] - Switching on/off electronic keys

-     [  idA  ] - Registration of electronic keys by users

-     [ nbL  ] - Block number

-     [ Pnu  ] - Range shift

-     [ LPi   ] - Amount of rooms on the floor

-     [ LLo  ] - Range of serviced numbers ( low value)

-     [ LHi  ] - Range of serviced numbers ( high value)

-     [ LdP  ] - Directing of not serviced numbers

-     [ rES  ] - Select the frequency of automatic restarts

-     [PrEd] - PR input operating mode selection

-     [  Un   ] - Additional number not included in the serviced range

# Lock codes / Locks Options

-     Physical number

-     Logical number

-     Lock code

-     Melody Nr.

-     Volume

-     Rings Nr.

-     Mode

-     Authorization

-     Lock code

# Electronic keys

-     Addition electronic key

-     Verification electronic key

-     Deleting electronic key

# Divided by subject

-     Numbering modes

-     Code of coded lock

-     Supply of camera and illumination

-     Blocking  of video signal

-     Electro-catch

-     Calling options

-     Automatically activation of electro-catch

-     User blockade

-     Electronic keys

## Serial number

A unique serial number of the processor, according to which computes an array of electronics in the cassette lock codes. It is printed on a sticker on the processor.
You can edit it, which is useful for example in the case of edition operation mode of electronic cassette from U to H. It can take values from 0000 to 9999. If in the number is the digit 0, then it must also be entered.
Parameter changes can be made insection [ System parameters – grouped by functionality ].

top of page

## Administrator password

Default administrator password is the serial number printed on a sticker on the processor.
You can edit it in the ISD-02 program. It can take values from 0000 to 9999. If in the the number is the digit 0, then it must also be entered.
NOTE!
If you forget password, then without interface ISD-02 and ISD-02 program it is impossible to retrieve it and it will be necessary to restore the default settings electronic cassette, which involves the loss of all entered settings.
Administrator password can be changed in section [ System parameters – grouped by functionality ].

top of page

## Data type identifier

Since version 6.7 software of electronic cassette in EEPROM memory is saved a special identifier that identifies system type, software version and operation mode of electronic cassette ( U or H ). Data type identifier allow self identification of electronic cassette type during receiving data from the EEPROM memory to ISD-02 program.
NOTE!
During each process of receiving data from the EEPROM memory of it should be noted that the program correctly determined the electronic cassette type. In the case of an erroneous reading, set the parameter [Data type identifier] by yourself.

Data type identifier is composed of:

- first digit define operation mode of electronic cassette
  - 0 - subordinate entrance ( U ),
  - 1 – main entrance ( H ),
- next two digits identify the type of system
  - 52 – system CD-2502
  - 31 – system CD-3100
- last two digits indicate the version of the software –e.g. 65, 66, itp.

top of page

## Object Identifier/ Installation addresss

addresss or name of the object, in which the electronic cassette is installed. Parameter help more easily identify the data and the files.
Name can contain 20 characters.
During saving data into files it will be default name of file -e.g.

3100_H70_1234_Dabrowskiego 249.bin
To change value [ Object Identifier/ Installation address] in section [ System parameters – grouped by functionality ].

top of page

## [EtYP] - Operation mode of electronic cassette

Parameter defining operation mode of electronic cassette:

- 0 - subordinate entrance - U
- 1 - main entrance - H

In a system with entrance hierarchy there are two types of entrances: the main entrance and subordinate entrances. System CD-2502 can operate for one main entrance and max. 64 subordinate entrances. From the main entrance a connection can be made with each apartment in any building or staircase serviced by the entry phone system. Using panels at the entrance to staircase (subordinate entrance) a connection can be made with the apartments located in this staircase only. Entry phones at subordinate entrances can be used independently. Default setting of the cassette is configured to operate with the subordinate entrance (U).

NOTE!
The parameter is not editable! To change the mode cassette electronics - see Menu/Instruction section Changing the Operation mode of electronic cassette.

top of page

## [ EAu] - Sound signal of sign selected from the keyboard

If this parameter is [ On ], then selection of any sign from the keyboard may be signalized with short acoustic signals heard on the speaker panel.

top of page

## [ ton] - Multitone signalling of sign selected from the keyboard

If this parameter is [ Off ], then selection of a key may be signalled with the same sound (one tone signalling) or (if [ ton ]=[ On ]) for every key sound of different pitch may be attributed (multitone signalling). The use of this function requires fulfilling the following condition [ EAu ]=1 and [ ton ]=1.

top of page

## [ dJ] - dJ

Duration of acoustic signal which signals selection of any sign from the keyboard is as long as time of keystroke but no longer then 1 second.
The use of this function requires fulfilling the following condition [ EAu ] and [ ton ].
Parameter was add in version 6.6 software of electronic cassette.

top of page

## [ CAon] - Supply of camera and illumination

Supply of camera and illumination

- Normal Mode - [ Off ]
Supply of camera and illumination of camera in external panel is turn on only during the conversation. Users can not monitor picture from camera.
- Continuously mode - [ On ]
Supply of camera and illumination of camera in external panel is continuously. If users want to monitor picture from camera also in the night, than the illumination of camera should be turn on continuously.

NOTE!
Even if illumination of camera is turn on continuously, it will be turn off automatically by photoelement in case of good enough external illumination.

top of page

## [ CAin] - Supported video inputs

This parameter specifies the type of change-over switch CVP witch is used, and defines supported by the CVP video signals displayed on the monitor screen of entry phone CD-2502 during switching

- Setting this parameter to value [0] makes that electronic cassette EC-2502 cooperates with change-over switch CVP-1.
- Setting this parameter to value higher than 0 makes that electronic cassette EC-2502 cooperates with change-over switch CVP-P-2,where the digits ( number from the range 1 - 1234 ) defining number of activated input in change-over switch.

Activating supported video inputs means that in the monitor screen switching on the preview screen will be activated sequentially between input signals. Switchover will take place at a certain period of time defined in the parameter [ CAtP]. Example:
[ CAin]= 124 - defines the switching between video signals:

- 1 - signal from the video camera in external panel at the main entrance H,
- 2 - signal from the video camera in external panel at the subordinate entrance (staircase) U
- 4 - signal from the additional video camera nr 4

top of page

## [ CAtP] - Switching picture time interval [s]

Parameter specifies the interval (time interval) in seconds between each switched signal from the video camera. Can be in the range 1-10

top of page

## [ 3C] - Switching on three-position display

Function should be switched on [ On ] when electronic cassette EC-2502 cooperates with the panel with three position of old type. In such case some messages appearing on the display will be distorted. Switching on the three position service makes that some messages appearing on the display will be diffrent from those described in the instruction.

top of page

## [ tOc] - Waiting time for picking up the receiver in seconds

Parameter defines waiting time for receiver pick up in seconds after finishing of calling.

top of page

## [ tro] - Time of conversation

Time of conversation between external panel user and uniphone user.
Conversation time after picking up the receiver is limited.10 s before the lapse of conversation programmed time sound signals will be heard in the receiver, which will inform about approaching time of breaking.

top of page

## [ trY] - Time of electro-catch operation in second [s]

Time of electrocatch operation in second [s].

top of page

## [ FrY] - Frequency of electro-catch supply voltage [Hz]

Electro-catch supplied with alternating voltage from a transformer makes a characteristic sound (humming) which is often associated with opening of door. This parameter makes it possible to simulate the operation of an electro-catch.
Entering value [ 0 ] makes that an electro-catch will operate without making any sound.
NOTE!
Electromagnetic lock should be supplied by voltage 12 V DC/1A.[ FrY] = [ 0 ]!

top of page

## [ APo ] - Acoustic confirming opening the electrocatch

If parameter [ APo ] in section [ System parameters – grouped by functionality → Door opening parameters ] or [ Parameters – order according to the system → Numerical parameters ] is set up on value [ 1 ] each opening of electro-catch will be signalized in external panel by acoustic signal.

top of page

## [ Ent ] - 'Fast entrance'

Entry phone CD-2502 realizes functions "fast entrance" which is used only in entry phone with the main and subordinate entrances.
In entry phone without this function one must ring the occupant twice in order to get to his apartment (the first time at the main entrance and the second time at the entrance to the staircase). Function "fast entrance" eliminates the second step.

top of page

## [ CEn] - Switching on coded lock service

Setting parameter [ CEn ] to [ Off ] value makes that function of coded lock will be switched off for all users regardless of setting for the individual apartments.
If parameter is set to [ On ] is possible switched off that function for indywidual users in section [ Lock codes / Locks Options ] setting parameter [ Lock code ] to "[-] - Off".

top of page

## [ CEd ] - Permission to edition of coded lock codes by occupants

Default [ CEd ] is set to [ On ] - the occupants have the possibility to change the codes of a combination lock in user's menu. Setting this parameter to value [0] blocks this possibility to all occupants regardless of individual settings.
If parameter [ CEd ] is [ On ] is possible to indywidual blocking edition of coded lock codes by occupants in section [ Lock codes / Locks Options ] by changing parameter [ Lock code ] to "[ E ] - Act.+Edition".
NOTE !
Edition by user is possible ONLY in subordinate entrance ( U ).

top of page

## [ CPo ] - Permission to confirm the use of lock code

Each unblocking of door by means of a coded lock makes that three short acoustic signals are generated in a uniphone mounted in an apartment whose code was used to open the door.
Parameter set to [0] enables to switch off this signalization in all uniphones. The Signalling can be switched off for the selected numbers.

top of page

## [ CEr ] - Confirming the use of a wrong code of coded lock

Entering the wrong code to a combination lock makes that two long acoustic signals will be generated in a uniphone mounted in an apartment to which there was an attempt to use a code to open the door. This is a signal for occupants that somebody tries to break the code of a combination lock.
This option ([ CEr ]=[ Off ])allows switching off this signalization in all uniphones.

top of page

## [ CHA ] - Request to enter code of coded lock during entering user's menu

Setting parameter value to [ On ] forces to enter the code of coded lock during entering user's menu.

top of page

## [ idE] - Switching on/off electronic keys

In section [ System parameters – grouped by functionality → Code lock parameters] or [ Parameters – order according to the system → Bit Parameters ] default value parameter [ idE ] is [ On ] - function of coded lock is switched on for all users.

top of page

## [ idA] - Registration of electronic keys by users

In a system is possible registration of electronic keys by users. Setting parameter [ idA ] value to [ On ] in section [ System parameters – grouped by functionality → Code lock parameters] or [ Parameters – order according to the system → Bit Parameters ] permits users to register new electronic keys from user's menu.

top of page

## [ nbL ] - Mode with building numbering

Switches on the mode with the building numbering. This numbering mode can be used only in entry phone system with entrance hierarchy (main entrance and subordinate entrances). This numbering mode allows repeating apartment numbers in different buildings.
In electronic cassette for subordinate entrance set parameter [ nbL ] (block number) to value higher then zero.
The operation should be repeated for other staircases (buildings). Values [ nbL ] can be repeated in subordinate systems provided that these systems operate with other logical numbers of uniphones.
In order to get connection with an apartment from an external panel at the main entrance one should first of all select building number and then apartment number.

In electronic cassette for main entrance set parameter [ NbL ] to value [ On ].

top of page

## [ Pnu ] - Range shift

Setting parameter [ Pnu ] to value higher then 0 switching on numbering mode with range shift.
In this numbering mode physical number of a uniphone (programmed by jumpers) differs from its logical number (under which a uniphone rings after having selected the number from the keyboard).
This numbering mode is used for apartments of numbers higher than 255.

logical number = physical number + range shift
Example:
In a building an entry phone should be used for apartments Nos. 301...310.
In uniphones physical numbers should be programmed as follows: in apartment 301 number 1, in apartment 302 number 2 etc.
Then parameter of range shift [ Pnu ] should be set to value 300.
After having done this and selecting from a keyboard number 301 the uniphone in which number 1 has been programmed will ring, after having selected number 302 uniphone with number 2 will ring etc.

top of page

## [ LPi ] - Amount of rooms on the floor

Setting parameter [ LPi ] to value higher then 0 switching on hotel numbering mode.
This numbering mode is meant for the buildings in which room number starts with a digit defining number of floor on which the room is located (hotels, resort houses, dormitories etc.).
Physical number of a uniphone is calculated according to the formula:

Physical number = P * LL + XX
where
P - floor number,
LL - amount of rooms on one floor (value of parameter [ LPi ])
XX - number of room on the floor ( number from the range 1 ... [ LPi ])

top of page

## [ LLo ] - Range of serviced numbers ( low value)

Parameter is used to set number range which is serviced by an entry phone. After selecting a number outside this range a message will appear on the display [ OFF ].
Limiting the range is recommended especially in case of an entry phone in a multi-entrance version.
Be careful that [ LLo ] < [ LHi ]. Otherwise selecting of any number will result in displaying a message [ OFF ].

top of page

## [ LHi ] - Range of serviced numbers ( high value)

Parameter is used to set number range which is serviced by an entry phone. After selecting a number outside this range a message will appear on the display [ OFF ].
Limiting the range is recommended especially in case of an entry phone in a multi-entrance version.
Be careful that [ LLo ] < [ LHi ]. Otherwise selecting of any number will result in displaying a message [ OFF ].

top of page

## [ LdP ] - Directing of not serviced numbers

All numbers which are not serviced by entry phone CD-2502, will be directed to uniphone number given as [ LdP ] value

top of page

## [ rES ] - Select the frequency of automatic restarts

Allows you to set how many hours the EC cassette will restart. Setting a value greater than 0 enables cyclic cassette restart. After 1 minute from setting the parameter, a trial restart is performed. Each next one is carried out in accordance with the set schedule.

top of page

## [PrEd] - PR input operating mode selection

PR input operating mode selection:

- Active level - [ Off ]
The low level of the signal at the PR input is active
- Active edge - [ On ]
The falling edge of the signal at the PR input is active

top of page

## [ Un ] - Additional number not included in the serviced range

n — number from the range 241...254

In many cases it is necessary to operate numbers which do not belong to the operated range.
For each of numbers [ Un ] it is possible to set individually any number from the range 1...9998.
NOTE !
If additional number will be the same as number that is already used, then the physical number that is assigned to this additional number will have a priority. This also applies to all individual settings.

top of page

# Divided by subject

## Numbering modes

Digital entry phone as a standard can operate numbers within a range 1...255 (Normal mode), however, very often it is necessary to operate higher numbers or numbers of considerably wider range. This is possible owing to different numbering modes:

- Numbering mode with range shift
- Hotel numbering mode
- Mode with building numbering

### Physical number

Number of uniphone (programmed by jumpers) within a range 1...255.

### Logical number

Number under which a uniphone rings after having selected the number from the keyboard - within a range 1...9998.

### Normal mode

In normal mode physical number of uniphone (programmed by jumpers) corresponds to logical number (selected from the keyboard of talking cassette). This is a default mode of operation of entry phone exchange.

### Numbering mode with range shift

In this numbering mode physical number of a uniphone (programmed by jumpers) differs from its logical number (under which a uniphone rings after having selected the number from the keyboard).
This numbering mode is used for apartments of numbers higher than 255.
Physical number of a uniphone is calculated according to the formula:

logical number = physical number + range shift
This numbering mode is switched on in a moment of setting of parameter [ Pnu ] to the value higher than [0].
Example:
In a building an entry phone should be used for apartments Nos. 301...310.
In uniphones physical numbers should be programmed as follows: in apartment 301 number 1, in apartment 302 number 2 etc.
Then parameter of range shift [ Pnu ] should be set to value 300.
After having done this and selecting from a keyboard number 301 the uniphone in which number 1 has been programmed will ring, after having selected number 302 uniphone with number 2 will ring etc.

### Hotel numbering mode

This numbering mode is meant for the buildings in which room number starts with a digit defining number of floor on which the room is located (hotels, resort houses, dormitories etc.).
Physical number of a uniphone is calculated according to the formula:

Physical number = P * LL + XX
where
P - floor number,
LL - amount of rooms on one floor (value of parameter [ LPi ])
XX - number of room on the floor, number from the range (1 ... [ LPi ])

This numbering mode will be activated at the moment of setting the value of parameter [ LPi ] to value higher than zero.

### Mode with building numbering

This numbering mode can be used only in entry phone system with entrance hierarchy. This numbering mode allows repeating apartment numbers in different buildings.
In order to get connection with an apartment from an external panel at the main entrance one should first of all select building number and then apartment number.
In electronic cassette for subordinate entrance set parameter [ nbL ] (block number) to value higher then zero and in electronic cassette for main entrance parameter [ NbL ] to value [ On ].
Values [ nbL ] can be repeated in subordinate systems provided that these systems operate with other logical numbers of uniphones.

### Additional numbers

In many cases it is necessary to operate numbers which do not belong to the operated range.
For each of numbers [Un] it is possible to set individually any number from the range 1...9998.
NOTE !
If additional number will be the same as number that is already used, then the physical number that is assigned to this additional number will have a priority. This also applies to all individual settings.

### Range of operated numbers(logical)

- [ LLo ] - Range of serviced numbers ( low value) - Physical number representing the low value of the range.
- [ LHi ] - Range of serviced numbers ( high value) - Physical number representing the high value of the range.

In default setting the operation of all apartment numbers is included. If the range is limited (parameters [ LLo ] and [LHi ] ), selection of a number outside the set range will result in displayed message [ OFF ].
Be careful that[ LLo ] < [ LHi ]. Otherwise selecting of any number will result in displaying a message [ OFF ]. Limiting is set for physical not logical numbers!
Default set range 1...240.

### Directing of not serviced numbers

All numbers which are not serviced by entry phone, will be directed to uniphone number given as [ LdP ] value

top of page

## Code of coded lock

To each apartment one four digital number is attributed which is preliminary defined in the entry phone production process.
To activate this function set parameter [ CEn ] to [ On ]. Function of coded lock will be switched on for all users regardless of setting for the individual apartments.
Code of coded lock can be changed by installing specialist or user (if parameter [ CEd ] is set to [ On ]).
Code of coded lock are declared only in the subordinate entrance cassette (U).

### Confirming the use of code of coded lock

Each unblocking of door by means of a coded lock ( correctly or wrongly) makes that acoustic signals are generated in a uniphone mounted in an apartment whose code was used to open the door.

- [ CPo] - Confirming the use of correctly code of coded lock - three short acoustic signals
- [ CEr] - Confirming the use of wrongly code of coded lock - two long acoustic signals

Parameter set to [0] enables to switch off this signalization in all uniphones. The Signalling can be switched off for the selected numbers.

### changing the code of coded lock

In section [ Lock codes / Locks Options ] can be change codes of coded lock for individual users.
NOTE !
In the interests of the existing electronic cassettes the program does not allow to restore the default codes of coded lock.
It would be enable to generate the correct code of coded lock by any other person. Therefore, restoring the default code of coded lock is only possible from the configuration procedures in electronic cassette.

### Special cods

There isn't special cods dedicated for postmen, administration. Special codes can be attributed to one of additional numbers: [Un] or to number witch isn't use by anyone.

### Individual settings - edition by users

Parameter [Lock code] - Options of combination lock for indywidual users:

- "[ - ] - Off" - Combination lock switched off
- [ A ] - Active - Combination lock activated, occupant can neither change the code or register electronic keys
- [ E ] - Act. + Edition - Combination lock activated, occupant may change the code and register electronic keys

in section [ Lock codes / Locks Options ].

### Request to enter code of coded lock during entering user's menu

Setting parameter [ CHA ] value to [ On ] forces to enter the code of coded lock during entering user's menu.

The request can be switched off for the selected numbers.

top of page

## Supply of camera and illumination

### Normal mode

Supply of camera and illumination of camera in external panel is turn on only during the conversation. Users can not monitor picture from camera.This is default mode - parameter [ CAon ] in section [ System parameters – grouped by functionality → Video signal service options ] or [ Parameters – order according to the system → Bit Parameters ] has value [ OFF ]. If users want to monitor picture from camera continuously [ CAon ] should be set to [ On ].

### Continuously mode

Supply of camera and illumination of camera in external panel is continuously. If users want to monitor picture from camera also in the night, than the illumination of camera should be turn on continuously. In section [ System parameters – grouped by functionality → Video signal service options ] or [ Parameters – order according to the system → Bit Parameters ] parameter [ CAon ] should be set to [ On ].
NOTE!
Even if illumination of camera is turn on continuously, it will be turn off automatically by photoelement in case of good enough external illumination.

top of page

## Door opening parameters

### Time of electro-catch operation in second [s]

Time of electrocatch operation [ trY ] can be set in section [ System parameters – grouped by functionality → Door opening parameters ] or [ Parameters – order according to the system → Numerical parameters ].

### Frequency of electro-catch supply voltage [Hz]

Entering value [ 0 ] to parameter [ FrY ] in section [ System parameters – grouped by functionality → Door opening parameters ] or [ Parameters – order according to the system → Numerical parameters ] makes that an electro-catch will operate without making any sound.
Entering value diffrent then [ 0 ] makes a characteristic sound (humming) which is often associated with opening of door.
Since version 6.7 software of electronic cassette - first 250ms always DC.
NOTE!
Electromagnetic lock should be supplied by voltage 12 V DC/1A.[ FrY] = [ 0 ]!

### 'Fast entrance'

Entry phone CD-2502 realizes functions "fast entrance" which is used only in entry phone with the main and subordinate entrances.
In entry phone without this function one must ring the occupant twice in order to get to his apartment (the first time at the main entrance and the second time at the entrance to the staircase). Function "fast entrance" eliminates the second step. To activate this function - in section [ System parameters – grouped by functionality → Door opening parameters ] or [ Parameters – order according to the system → Bit Parameters ] change parameter [ Ent ] to 1.

top of page

## Calling options

Calling signal consists of several parts:

- Calling signal – multiplicity of parameters:
  - Time of individual tone generation [ t1t ] - consists of three tones of different frequency F0 (1 kHz), F1 and F2
  - Time of signal generation [ t1d ]
  - Pause time between successive signals ( if number of bells are set to more then 1) [ tPA ]
  and
- Waiting time for picking up the receiver [ tOC ]

Parameters: number of bells, calling ton, calling volume can be set for indywidual users. Signal frequency, time of individual tone generation, pause time, waiting time for picking up the receiver are global parameters for all users conected to this electronic cassette.

### [ t1d ]

Time of signal generation [*10ms] consists of signals [ t1t ] of different frequency.

### [ tPA ]

Pause time *10[ms] after signal [ t1d ]

### [ tOc ]

Waiting time for picking up the receiver in seconds

### Melody Nr.

Parameter can take values from the range 0...7. Parameter value is defined by one of 8 pre-defined calling tones.

### Volume

Entry phone enables setting three volume levels and calling of increasing volume (requires setting at least two bells):

- [C] - silent bell
- [U] - moderate bell
- [G] - loud bell
- [N] - increasing bell.

### Rings Nr.

Parameter can take values from the range 0...7.

top of page

## Authorization

In the entry phone it is possible to define how the pushbutton operates the electro-catch at the individual entrances:

- [-] - blockade - No electro-catch control from the uniphone (monitor)
- [U] - only U - Pushbutton activates electro-catch at the subordinate entrance only
- [H] - only H - Pushbutton activates electro-catch at the main entrance only
- [A] - U+H - Pushbutton activates electro-catch at the main entrance and at the subordinate entrance
- [d] - U+H auto. - Pushbutton activates electro-catch at the main entrance and at the subordinate entrance. Additionally if the receiver is picked up, then entering the number of this uniphone will activate electro-catch automatically.
- [b] - video block. - blocking video signal during connection

top of page

## Automatically activation of electro-catch

It is possible to open electro-catch after pick up the receiver automatically. To activate this option it is needed to select in section [ Lock codes / Locks Options ] parameter [ Authorization ] to [d] - U+H auto.

top of page

## User blockade

It is possible to limit possibility of opening entrances, possibility of talking or blocking the uniphone.

### possibility of opening entrances

Switching off possibility of opening entrances - setting parameter [Authorization] in section [ Lock codes / Locks Options ] to "[ - ] - Off".
It is possible to limit selectively possibility of opening entrances (U orH):

- [A] - Pushbutton activates electro-catch at the main entrance and at the subordinate entrance [ U + H ],
- [H] - Pushbutton activates electro-catch at the main entrance only ,
- [U] - Pushbutton activates electro-catch at the subordinate entrance only

NOTE !
User can change parameter in USER'S MENU

### Blocking possibility of talking (uniphone functions as a bell)

Uniphone may be called, however, conversation cannot be conducted and electro-catch cannot be controlled. Blockade will be activated after changing parameter [Mode] in section [ Lock codes / Locks Options ] to "[d]- Bell".
NOTE !
User can change parameter in USER'S MENU

### Uniphone blockade

Uniphone switched off. Changing parameter [Mode] in section [ Lock codes / Locks Options ] to "[ - ] - Off" makes that it is impossible to make a connection with the apartment for which such setting was selected. An attempt to make a connection will be followed by a message [ OFF ] .
NOTE !
User can not change parameter in USER'S MENU

top of page

## [Mode]

If needed entry phone reaction after calling can be changed:

- [ - ]- Off - Uniphone switched off
- [ d ]- Bell - Blocking possibility of talking (uniphone functions as a bell)
- [ A ]- Active - Active uniphone
- [ P ]- Act - Conf - Active uniphone. Uniphone may be called, conversation can be conducted and electro-catch may be controlled. There is no confirmation of use of lock code and electronic keys.

Parameter can be changed in section [ Lock codes / Locks Options ].

top of page

## Electronic keys

Entry phone CD-2502 can be equipped with electronic key reader. There are three kinds of keys in entry phone:

- service keys enable change of entry phone configuration,
- special keys are used by postmen, administration etc.
- keys for the occupants.

Keys should be registered at both the main and subordinate entrance. At the main entrance keys attributed to apartment cannot be registered. Entry phone users can register their own electronic keys. This possibility can be switched on globally by setting parameter [ idA] to value [ On ].

- Switching on electronic key
  Default value parameter [ idE] is [ On ] - users can register their own electronic keys. In another case, parameter [ idE] should be changed in main and subordinate entrance electronic cassette.
- Registration of electronic keys by users
  In a system is possible registration of electronic keys by users. Setting parameter [ idA] value to [ On ]

### Addition

ISD-02 interface allow registration electronic keys in electronic cassette, addition of keys with attributing to apartment, addition on the selected item in memory, and copying keys ( all or whole section) from one electronic cassette to other, or saving settings in file. Using program ISD-02 it is possible to write and read data to the table to / from a file with the extension *.tm, that is so after programmed keys in one electronic cassette it is easily to copy it to another located in the system (for example, to copy from subordinate entrance cassette tapes to main entrance cassette). To save the table select in section [ Electronic keys ] the area you want to copy and press the right mouse button and choose [ Save to file ], and give it a name. To load data into an table, press the right mouse button in the line of the table and choose [ Import from file ].
NOTE !
The data that we import from the file will be inserted into the cell line which pointed out. Data in the table will be replaced data imported from the file.
Example:
In file is 12 keys, if we paste them from position 100 then data from positions 100-111 will be deleted and replaced by new. Saved file can be edited. To make change it should be opened in any program to text edition (eg. notepad) made data changes, and finally file must be saved
Besides addition keys by installing specialist it is possible addition keys by users after setting parameter [ idA] to [ On ].

The program allows addition:

#### One electronic key

If you want to add one electronic key, then in section [ Electronic keys ] choose [ Add ] and apply key to the reader ISD. The serial number of electronic key will bereading and show in the box [Serial Number]. This key will be add to first free position. If this key was earlier registrated it will not be add – line with this particular key will be highlighted.

#### Several keys at once

If you want to add several keys at once, then choose [ Add ] and apply all keys successively to the reader ISD. They will be successively added to the first free position.

#### Addition to Flat

If you want to add one electronic key to particular flat, then in section [ Electronic keys ] choose [ Add to Flat ], write number of this flat and apply key to the reader ISD. Electronic key will be add to first free position.

#### Addition to Position

If you want to add one electronic key to particular position, then in section [ Electronic keys ]:

- select the position of the cursor,
- choose [ Add to Position ]
- apply key to the reader ISD.

### Verification

#### Verification the key is already registered in the system

If you want to verify that the key is already registered in the system - in section [ Electronic keys ] choose [ Verify key ] and apply key to the reader ISD. If this key was earlier registrated line with this particular key will be highlighted.

#### Verification the key is already registered in the flat

If you want to verify that the key is already registered in specific flat - write number of this flat and choose [ Find flat ]. In box [ Position ] will be specify numbers of positions where is this number of flat. After mark this position and double pressing of left button on mouse line with this particular flat will be highlighted.

### Registering one key in several electronic cassettes

There is possibility of addition one key to several electronic cassette (eg. several subordinate entrances and one main entrance, or only to subordinate entrances). For postmen, administration etc. aside an area designated numbers 1000-1019, which can select and save the file, and during programming other electronic cassette import selected area table to area designed for special keys used by postmen, administration etc. in section [ Electronic keys ].

### Deleting key

Deleting the key from memory will take place after marking line with key and pressing on the keyboard 'Delete'. Deleting all keys from memory will take place after marking any cell in the table and pressing at the same time 'ctrl' and 'a'on the keyboard and next 'Delete'.

top of page

###### v1.0 (24-11-2010)