<!-- This comment will put IE 6, 7 and 8 in quirks mode -->
<!-- <!DOCTYPE html PUBLIC "-//W3C//DTD XHTML 1.0 Transitional//EN" "http://www.w3.org/TR/xhtml1/DTD/xhtml1-transitional."> -->
<html xmlns="http://www.w3.org/1999/xhtml">
<head>
<meta http-equiv="Content-Type" content="text/xhtml;charset=UTF-8"/>
<title>ISD-02 - configuration of digital entry phone system made by Laskomex </title>
<link href="styl.css" rel="stylesheet" type="text/css"/>
</head>
<body style=" background-image: url(tlo_isd_rfid2.jpg); background-repeat: repeat;"> 
<h3><a name="home">Version 1.1 (09-03-2011)</a></h3>
<div id="wrap">
<!--<h1 class="title"><a href="#a.html" name="home">PROGRAM DO KONFIGURACJI DOMOFONÓW CYFROWYCH FIRMY LASKOMEX</a></h1>-->
<p class="fota2"><img src="ISDLOGO.jpg" width="688" height="199" border="0" alt="[ISDLOGO.jpg]" /></p>
<!-- ================================================================================================ -->
<div id="menutop">
<a href="welcome.html">|Start page|</a>
</div>


<ul class="menu">
	<li><a href="#przeznaczenie">Destination of program</a></li>
	<li><a href="#wymagania">Hardware requirements</a></li>
	<li><a href="#zawartosc">Kit contents</a></li>
	<li><a href="#instalacja">Installation of software</a></li>
	<li><a href="#struktura">Catalog structure of software</a></li>

	<li style="list-style: none"><a name="home">&nbsp;</a></li>

	<li><a href="#interface">User interface - GUI</a></li>
	<ul>
		<li><a href="#panelinterface">"Interface" panel</a></li>
		<li><a href="#panelpamiec">"Memory device" panel</a></li>
		<li><a href="#panelkomputer">"PC" panel</a></li>
	</ul>
	<li><a href="#skroty">Keyboard shortcuts</a></li>
	<li><a href="#opiszakladek">Description of tabs</a></li>

	<li style="list-style: none"><a name="home">&nbsp;</a></li>

	<li><a href="#polaczeniezcetrala">Connection with EC electronic cassette</a></li>
	<li><a href="#wymianadanych">Exchange of data using MLX module</a></li>
	<ul>
		<li><a href="#pamiecwewnetrzna">Internal memory</a></li>
		<ul>
			<li><a href="#ecgolasko">EC - MLX connection</a></li>
			<li><a href="#n1">MLX - ISD-02 connection</a></li>
		</ul>
		<li><a href="#n2">DIP memory</a></li>
	</ul>
	<li style="list-style: none"><a name="home">&nbsp;</a></li>

	<li><a href="#n3">Receiving data from memory</a></li>
	<li><a href="#n4">Restoring default settings</a></li>
	<li><a href="#n5">Import/export data from/to file</a></li>
	<ul>
		<li><a href="#n6">Export to *.op and *.id file</a></li>
		<li><a href="#n7">Import from *.op and *.id file</a></li>
	</ul>
	<li><a href="#n8">Copying/pasting data area</a></li>
	<li><a href="#n9">Edition of electronic key</a></li>
	<ul>
		<li><a href="#dodawanietm">Addition of electronic key</a></li>
		<ul>
			<li><a href="#a1">without assigned to the apartment</a></li>
			<li><a href="#a2">with assigned to the apartment</a></li>
			<li><a href="#a3">on the selected item in memory</a></li>
		</ul>
		<li><a href="#a4">Searching for electronic key assigned to specific apartment</a></li>
		<li><a href="#a5">Checking for electronic key applied to ISD-02 interface</a></li>
	</ul>
	<li><a href="#a6">Changing electronic cassette operation mode</a></li>
	<ul>
		<li><a href="#a7">Changing mode from U to H</a></li>
		<li><a href="#a8">Changing mode from H to U - requires support in external panel</a></li>
	</ul>
	<li><a href="#a9">Copying databases of electronic keys from few U electronic cassettes to H one</a></li>
</ul>

<br /><br /><br /><br /><br /><br /><br /><br /><br /><br /><br /><br /><br /><br /><br /><br />

<!-- ================================================================================================ -->
<div class="ha1">
<h2><a name="przeznaczenie">Destination of program</a></h2>
  ISD-02 software is used to configure all the parameters of CD-2502 and CD-3100 entry phone system, and database management of identifiers - electronic keys "iButton" or
  "RFID" (125kHz standard).

<p class="ret"><a href="#home">Back</a></p>	
</div>

<!-- ================================================================================================ -->
<div class="ha2">
<h2><a name="wymagania">Hardware requirements</a></h2>
<ul>
	<li>PC equipped with minimum 400MHz processor and 256MB RAM</li>
	<li>CD-ROM drive + 100MB free disk space on hard drive </li>
	<li>minimum screen resolution 800x600</li>
	<li>1 free USB 1.1 or 2.0 port to connect ISD-02 interface</li>
	<li>mouse or other pointing device</li>
	<li>one of the operating systems: Windows 7, Windows XP or Linux (Ubuntu 9.1 version)</li>
</ul>

<p class="ret"><a href="#home">Back</a></p>	
</div>
<!-- ================================================================================================ -->
<div class="ha1">
<h2><a name="zawartosc">Kit contents</a></h2>
<table width="100%" cellspacing="2" cellpadding="2" border="0" class="tabelka">
<tr class="jasny"><td>ISD-02 interface</td><td>1</td><td>pc.</td></tr>
<tr class="ciemny"><td>USB-A / USB-B mini cable</td><td>1</td><td>pc.</td></tr>
<tr class="jasny"><td>Cable to connect with electronic cassette</td><td>1</td><td>pc.</td></tr>
<tr class="ciemny"><td>MLX module</td><td>5</td><td>pcs.</td></tr>
<tr class="jasny"><td>CD with software</td><td>1</td><td>pc.</td></tr>
</table>



<p class="ret"><a href="#home">Back</a></p>	
</div>
<!-- ================================================================================================ -->
<div class="ha2">
<h2><a name="instalacja">Installation of software</a></h2>
Installation of ISD-02 software does not require specialized installer. One should just copy the appropriate directory to PC's hard drive. 
<ul>
<li> Depending on the installed operating system in the PC, one should copy from CD to PC's hard drive the entire contents of the ISD-02 directory: 
<table width="90%" cellspacing="2" cellpadding="2" border="0" class="tabelka2">
	<tr class="jasny"><td>for Windows operating system</td><td><b>SOFTWARE/WINDOWS/ISD-02/*.*</b></td></tr>
	<tr class="ciemny"><td>for LINUX operating system</td><td><b>SOFTWARE/UBUNTU/ISD-02/*.*</b></td></tr>
</table>
<!--<ul>
	<li style="list-style: none"><a name="home">&nbsp;</a></li>
	<li>	dla Windows XP		SOFTWARE/WinXP/ISD-02/*.*</li>
	<li>	dla Windows Vista	SOFTWARE/Vista/ISD-02/*.*</li>
	<li>	dla Windows 7		SOFTWARE/W7/ISD-02/*.*</li>
	<li>	dla systemu LINUX	SOFTWARE/LINUX/ISD-02/*.*</li>
</ul></li>-->

<li style="list-style: none"><a name="home">&nbsp;</a></li>
<li>In Linux operating system make sure that after copying to hard drive, files <b>isd.sh</b> and <b>ISD-02</b> have "<b>Allow executing file as program</b>" option selected in tab "<i>Permissions</i>" in "<i>Properties</i>".</li>

<li style="list-style: none"><a name="home">&nbsp;</a></li>
<li>Using supplied USB-A/mini USB-B cable, connect ISD-02 interface to the PC.</li>

<li style="list-style: none"><a name="home">&nbsp;</a></li>
<li>For Linux operating system installation process has come to an end - one should just copy the appropriate directory. The further part of the installation applies only to Windows 7 and Windows XP.</li>

<li style="list-style: none"><a name="home">&nbsp;</a></li>
<li>Windows operating system should detect connection of new device and display the window.
<br />
<br />

<b class="uwaga">NOTE!</b> <br/>
<i>For driver installation, Windows administrator rights are required.</i>
<br /></li>
<br /><br />

<p class="fota"><img src="img01.jpg" width="503" height="391" border="0" alt="[img01.jpg]" /></p>

<li>In displayed window one should select "<b>Install from a list or specific location</b>" option and press "<b>Next</b>" button</li>

<p class="fota"><img src="img02.jpg" width="500" height="389" border="0" alt="[img02.jpg]" /></p>

<li>In next window one should select "<b>Include this location in the search</b>" option and by pressing "<b>Browse</b>" button, specify the path to the <b>DRIVER</b> directory which is present in main ISD-02 directory. After specify the path, press "<b>Next</b>" button</li>

<p class="fota"><img src="img03.jpg" width="623" height="395" border="0" alt="[img03.jpg]" /></p>
<li>Windows operating system should display "<b>Hardware Installation</b>" window where one should press "<b>Continue Anyway</b>" button</li>

<p class="fota"><img src="img04.jpg" width="503" height="391" border="0" alt="[img04.jpg]" /></p>
<li>After finish driver installation a window should be displayed where one should press "<b>Finish</b>" button</li>

<p class="fota"><img src="img05.jpg" width="236" height="370" border="0" alt="[img05.jpg]" /></p>
<li>Driver installation was completed successfully. The device has been installed and assigned to the first available COM port (see Device Manager)</li>
</ul>

<p class="ret"><a href="#home">Back</a></p>	
</div>
<!-- ================================================================================================ -->
<div class="ha2">


<h2><a name="struktura">Catalog structure of software</a></h2>

<ul>
	<li>
	<b>ISD-02</b> - main directory 
	<ul>
	
	<li><b>APPLICATION</b> - directory with program files
	<ul>
	<li><b>MEDIA</b> - sound files</li>
	<li><b>PNG</b> - icons and graphics</li>
	<li><b>XML</b> - definitions of EC electronic cassettes </li>
	</ul> </li>
	
	
	<li><b>DATA</b> - directory with user data
	<ul>
	<li><b>INIT_EC</b>		- directory with standard data from electronic cassettes</li>
	<li><b>SUBDIVISION_A</b>		- example of directory with data from electronic cassettes
	<ul>
	<li><b>... *.bin</b>		- files with data from electronic cassettes</li>
	</ul>
	</li>
	<li><b>... *.bin</b>			- files with data from electronic cassettes</li>
	<li><b>... *.op</b>			- files with data of coded lock codes database and individually settings</li>
	<li><b>... *.id</b>			- files with data of electronic key databases</li>
	</ul></li>
	
	
	<li><b>DRIVER</b> - directory contains driver for ISD-02 interface - only in Windows operating system versions
	<ul>
	<li><b>ISD-02_XPV7.inf</b>	- driver file</li>
	</ul>
	</li>
	
	
	<li><b>HELP</b> - help files
	<ul>
	<li><b>APPLICATION </b>	- application help files
		<ul>
		<li><b>PL</b>		- for Polish language</li>
		<li><b>EN </b>		- for English language </li>
		<li><b>...</b>		- other languages</li>
		</ul>
	</li>
		<li><b>SYSTEM</b>		- help files for EC electronic cassettes
		<li><b>PL</b>		- for Polish language
		<ul>
		<li><b>EC2502_U65</b>  - help file for EC2502_U65 electronic cassette</li>
		<li><b>EC2502_H65</b>  - help file for EC2502_H65 electronic cassette</li>
		<li><b>...</b>	- other electronic cassettes</li>
		</ul>
	</li>
		<li><b>EN</b>		- for English language </li>
		<li><b>...</b>		- other languages</li>
		</ul>
	</li>

	</li>
	
	<li><b>LIB</b> - directory contains libraries - only in Linux operating system version
		<ul>
		<li><b>IMAGEFORMATS</b> - directory contains libraries supporting graphics
			<ul>
			<li><b>*.so</b> - libraries</li>
			</ul>
		</li>
		<li><b>*.so</b> - libraries</li>
		</ul>
	</li>
	
	<li><b>Laskomex_ISD-02.exe</b>	- executable file - only in Windows operating system versions</li>	
	
	<li><b>*.dll</b> - libraries - only in Windows operating system versions</li>
	
	<li><b>isd.sh</b>	- start-up script - only in Linux operating system version</li>
	
	<li><b>ISD-02</b>	- executable file - only in Linux operating system version</li>
	</ul>
	</li>
	</ul>
	</ul>

<p class="ret"><a href="#home">Back</a></p>	
</div>



<!-- ================================================================================================ -->
<div class="ha2">

<h2><a name="interface">User interface - GUI</a></h2>
<table width="100%" cellspacing="10" cellpadding="10" border="0" class="tabelka2">
<tr> <td><img src="img06.jpg" width="468" height="157" border="0" alt="[img06.jpg]" align="middle" /></td><td>Language selection</td></tr>
</table>
	
<p><img src="img07.jpg" width="755" height="113" border="0" align="bottom" alt="[img07.jpg]" /></p>

<p>The main panel of program</p>

<p class="ret"><a href="#home">Back</a></p>	
</div>




<!-- ================================================================================================ -->
<div class="ha1">
<h2><a name="panelinterface">"Interface" panel</a></h2>

<table width="100%" cellspacing="10" cellpadding="10" border="0" class="tabelka2">
<tr> <td><img src="foto17.jpg" width="228" height="102" border="0" alt="[foto17.jpg]" align="middle" /></td><td>Panel is used for finding and selection of serial COM port to which ISD-02 interface is connected to and for making connection with this interface.</td></tr>


<tr> <td><img src="foto35.jpg" width="108" height="29" border="0" alt="[foto35.jpg]" /></td><td>Finds an available COM ports</td></tr>


<tr> <td><img src="foto12.jpg" width="246" height="106" border="0" alt="[foto12.jpg]" /></td><td>
Selection list of device from which the connection is going to be made with</td></tr>


<tr> <td><img src="foto29.jpg" width="107" height="28" border="0" alt="[foto29.jpg]" /><br /><img src="foto13.jpg" width="107" height="29" border="0" alt="[foto13.jpg]" /></td><td>
Adequately establish or disconnect a connection to a device that is visible in the selection list.</td></tr>
</table>

<p>COM port to which ISD-02 interface is connected to has a following name: <br/>
"<b>COMxx ISD-02 HW-h/SW-f.w</b>", where</p>
<ul>
	<li><b>xx</b>	- means COM port number</li>
	<li><b>h</b> 	- means ISD-02 device version</li>
	<li><b>f.w</b> 	- means software version of ISD-02 interface</li>
</ul>

<p class="ret"><a href="#home">Back</a></p>	
</div>



<!-- ================================================================================================ -->
<div class="ha2">
<h2><a name="panelpamiec">"Memory device" panel</a></h2>

<table width="100%" cellspacing="10" cellpadding="10" border="0" class="tabelka2">
<tr> <td><img src="foto10.jpg" width="269" height="102" border="0" align="bottom" alt="[foto10.jpg]" /></td><td>Panel where memory type to exchange data can be choose.</td></tr>
</table>
<br />
<p>CD system configuration by ISD-02 may be carried out in three ways:</p>
<table width="100%" cellspacing="10" cellpadding="10" border="0" class="tabelka2">
<tr> <td><img src="foto27.jpg" width="88" height="53" border="0" alt="[foto27.jpg]" /></td><td>direct connection between EC electronic cassette and ISD-02 interface</td></tr>
<tr> <td><img src="foto09.jpg" width="86" height="52" border="0" alt="[foto09.jpg]" /></td><td>data exchange using internal memory in MLX module (backup/upload of data - support from panel's keyboard)</td></tr>
<tr> <td><img src="foto26.jpg" width="87" height="52" border="0" alt="[foto26.jpg]" /></td><td>read/write from/to DIP memory removed from EC electronic cassette and inserted to MLX module</td></tr>
</table>

<p>ISD-02 interface automatically detects the connected type of memory. 
If a button is <b class="szary">grey</b> it means, that specified memory is not connected to ISD-02 interface.</p>
<table width="100%" cellspacing="10" cellpadding="10" border="0" class="tabelka2">
<tr> <td><img src="foto16.jpg" width="131" height="28" border="0" alt="[foto16.jpg]" /></td><td>receiving data from the selected memory/device and displays them in program's editor.</td></tr>
<tr> <td><img src="foto18.jpg" width="130" height="28" border="0" alt="[foto18.jpg]" /></td><td>sending actually edited data to the selected memory/device.</td></tr>
</table>

<p class="ret"><a href="#home">Back</a></p>	
</div>





<!-- ================================================================================================ -->
<div class="ha1">
<h2><a name="panelkomputer">"PC" panel</a></h2>

<table width="100%" cellspacing="10" cellpadding="10" border="0" class="tabelka2">
<tr> <td><img src="foto14.jpg" width="300" height="99" border="0" align="bottom" alt="[foto14.jpg]" /></td><td>Buttons on this panel allow to save edited parameters to *.bin file on hard drive and load them. </td></tr>
</table>

<table width="100%" cellspacing="10" cellpadding="10" border="0" class="tabelka2">
<tr> <td class="cent"><img src="foto101.jpg" width="89" height="28" border="0" align="bottom" alt="[foto101.jpg]" /></td><td>- load data from "<b>*.bin</b>" file</td></tr>
<tr> <td class="cent"><img src="foto102.jpg" width="87" height="27" border="0" align="bottom" alt="[foto102.jpg]" /></td><td>- save current configuration to actually opened "<b>*.bin</b>" file</td></tr>
<tr> <td class="cent"><img src="foto103.jpg" width="103" height="28" border="0" align="bottom" alt="[foto103.jpg]" /></td><td>- save current configuration to "<b>*.bin</b>" file with the possibility of naming it</td></tr>
</table>

<p class="ret"><a href="#home">Back</a></p>	
</div>


<!-- ================================================================================================ -->
<div class="ha2">
<h2><a name="skroty">Keyboard shortcuts</a></h2>
<p>It is possible to navigate ISD-02 program without using pointing device -  by keyboard shortcuts:</p>

<table width="100%" cellspacing="5" cellpadding="5" border="0" class="tabelka2">
	<tr> <td><b>Left ALT+Z</b>	</td><td>	allows in "<b>Coded lock codes/Flats options</b>" tab to change the value of parameter for entire column</td></tr>
	<tr> <td><b>TAB </b>		</td><td>	forward shift between elements in the whole window</td></tr>
	<tr> <td><b>SHIFT+TAB</b>		</td><td>	backward shift between elements in the whole window</td></tr>
	<tr> <td><b>CTRL+TAB</b>	</td><td>	shift between tabs - does not work in main panel</td></tr>
	<tr> <td><b>TAB+Left ALT</b>	</td><td>	shift between working area and Menu strip</td></tr>
	<tr> <td><b>CTRL+A</b>	</td><td>	selection of all the cells in a table</td></tr>
	<tr> <td><b>CTRL+C</b>	</td><td>	copying the selected data area to the clipboard</td></tr>
	<tr> <td><b>CTRL+V</b>	</td><td>	pasting data from clipboard</td></tr>
</table>

<table width="100%" cellspacing="3" cellpadding="5" border="0" style="font-size: 10pt">

<tr style="background-color: #F7F7F7"><td class="cent"><img src="foto35.jpg" width="108" height="29" border="0" align="bottom" alt="" /></td><td width="500">Left ALT+P</td></tr>
<tr style="background-color: #E9E9E9"><td class="cent"><img src="foto29.jpg" width="107" height="28" border="0" align="bottom" alt="" />
			<img src="foto13.jpg" width="107" height="29" border="0" align="bottom" alt="" /></td><td>Left ALT+L</td></tr>
<tr style="background-color: #F7F7F7"><td class="cent"><img src="foto27.jpg" width="88" height="53" border="0" align="bottom" alt="" /></td><td>Left ALT+C</td></tr>
<tr style="background-color: #E9E9E9"><td class="cent"><img src="foto09.jpg" width="86" height="52" border="0" align="bottom" alt="" /></td><td>Left ALT+G</td></tr>
<tr style="background-color: #F7F7F7"><td class="cent"><img src="foto26.jpg" width="87" height="52" border="0" align="bottom" alt="" /></td><td>Left ALT+D</td></tr>
<tr style="background-color: #E9E9E9"><td class="cent"><img src="foto16.jpg" width="131" height="28" border="0" align="bottom" alt="" /></td><td>Left ALT+R</td></tr>
<tr style="background-color: #F7F7F7"><td class="cent"><img src="foto18.jpg" width="130" height="28" border="0" align="bottom" alt="" /></td><td>Left ALT+M</td></tr>
<tr style="background-color: #E9E9E9"><td class="cent"><img src="foto101.jpg" width="89" height="28" border="0" align="bottom" alt="" /></td><td>Left ALT+O</td></tr>
<tr style="background-color: #F7F7F7"><td class="cent"><img src="foto102.jpg" width="87" height="27" border="0" align="bottom" alt="" /></td><td>Left ALT+S</td></tr>
<tr style="background-color: #E9E9E9"><td class="cent"><img src="foto103.jpg" width="103" height="28" border="0" align="bottom" alt="" /></td><td>Left ALT+A</td></tr>
<tr style="background-color: #F7F7F7"><td class="cent"><img src="foto01.jpg" width="189" height="156" border="0" align="bottom" alt="" /></td><td>Left ALT+I</td></tr>
<tr style="background-color: #E9E9E9"><td class="cent"><img src="foto21.jpg" width="186" height="156" border="0" align="bottom" alt="" /></td><td>Left ALT+F</td></tr>
<tr style="background-color: #F7F7F7"><td class="cent"><img src="foto23.jpg" width="186" height="155" border="0" align="bottom" alt="" /></td><td>Left ALT+B</td></tr>
<tr style="background-color: #E9E9E9"><td class="cent"><img src="foto19.jpg" width="187" height="155" border="0" align="bottom" alt="" /></td><td>Left ALT+V</td></tr>
<tr style="background-color: #F7F7F7"><td class="cent"><img src="foto34.jpg" width="187" height="155" border="0" align="bottom" alt="" /></td><td>Left ALT+X</td></tr>
</table>

<!-- <table width="100%" cellspacing="2" cellpadding="2" border="0" class="tabelka">
<tr class="jasny"><td>ALT+P</td><td>Wyszukaj</td></tr>
<tr class="ciemny"><td>ALT+L</td><td>Połacz/Rozłącz</td></tr>
<tr class="jasny"><td>ALT+R</td><td>Odbierz</td></tr>
<tr class="ciemny"><td>ALT+M</td><td>Wyślij</td></tr>
<tr class="jasny"><td>ALT+O</td><td>Wczytaj</td></tr>
<tr class="ciemny"><td>ALT+S</td><td>Zapisz</td></tr>
<tr class="jasny"><td>ALT+A</td><td>Zapisz jako...</td></tr>
<tr class="ciemny"><td>ALT+C</td><td>System CD</td></tr>
<tr class="jasny"><td>ALT+G</td><td>MLX</td></tr>
<tr class="ciemny"><td>ALT+D</td><td>MLX DIP</td></tr>
<tr class="jasny"><td>ALT+I</td><td>menu/instrukcja</td></tr>
<tr class="ciemny"><td>ALT+F</td><td>menu/zakończ edycję</td></tr>
<tr class="jasny"><td>ALT+B</td><td>menu/wróć do edycji</td></tr>
<tr class="ciemny"><td>ALT+V</td><td>zakończ edycję</td></tr>
<tr class="jasny"><td>ALT+X</td><td>menu/zamknij</td></tr>
<tr class="ciemny"><td>ALT+Z</td><td>zakładce "Kody zamka/Opcje lokali" pozwala zmienić wartość parametru dla całej kolumny</td></tr>
<tr class="jasny"><td>TAB</td><td>przechodzenie pomiędzy kolejnymi elementami w całym oknie programu w przód</td></tr>
<tr class="ciemny"><td>SHIFT+TAB</td><td>przechodzenie pomiędzy kolejnymi elementami w całym oknie programu w tył</td></tr>
<tr class="jasny"><td>CTRL+TAB</td><td>przechodzenie pomiędzy zakładkami- nie działa w panelu głównym</td></tr>
<tr class="ciemny"><td>TAB+ALT</td><td>przechodzenie pomiędzy oknem programu a paskiem Menu</td></tr>
</table>
-->


<p class="ret"><a href="#home">Back</a></p>	
</div>


<!-- ================================================================================================ -->
<div class="ha1">
<h2><a name="opiszakladek">Description of tabs</a></h2>


<table width="100%" cellspacing="5" cellpadding="5" border="0" class="tabelka">
<tr class="jasny"><td><b>System parameters – grouped by functionality</b></td><td>Parameters available in electronic cassette in procedures P-1, P-2 and P-6 (change of administrator password), and parameters that identify electronic cassette (serial number, electronic cassette's data type ID, object ID) grouped into function blocks</td></tr>
<tr class="ciemny"><td><b> System parameters – order according to the CD system</b></td><td>Parameters available in electronic cassette in procedures P-1 and P-2 in order such as in electronic cassette</td></tr>
<tr class="jasny"><td><b>Coded lock codes/Flats options</b></td><td>Individual settings of occupants (P-5 procedure equivalent) and coded lock codes (P-9)</td></tr>
<tr class="ciemny"><td><b>Identifiers - electronic keys</b></td><td>Identifiers - electronic keys database (P-4 procedure equivalent)</td></tr>
<tr class="jasny"><td><b>Description of parameters - Manual</b></td><td>Description of parameters for actually edited type of electronic cassette and its software version</td></tr>

</table>

<p class="ret"><a href="#home">Back</a></p>	
</div>




<!-- ================================================================================================ -->
<div class="ha2">
<h2><a name="polaczeniezcetrala">Connection with EC electronic cassette</a></h2>

<table width="100%" cellspacing="5" cellpadding="5" border="0" class="tabelka">
<tr class="ciemny"><td><b>Newer type of electronic cassette - the connector is in the middle part of the PCB circuit</b></td></tr>
<tr><td><p><center><img src="ecisd.jpg" width="739" height="472" border="0" alt="[ecisd.jpg]" /></center></p></td></tr>
<tr class="ciemny"><td><b>Older type of electronic cassette - the connector is on the edge of the PCB circuit</b></td></tr>
<tr><td><p><center><img src="ecisd2v2.jpg" width="739" height="472" border="0" alt="[ecisd2v2.jpg]" /></center></p></td></tr>

</table>

<ul>
	<li>connect ISD-02 interface with EC electronic cassette using appropriate cable which is included to the kit</li><br/><br/>
	<p><b class="uwaga">NOTE!</b><br /> In case of an older type of electronic cassette the connection cable should be inserted only on the top row of pins.<br/>Coding inset in the plug should be at the top.<br/></p> 
	<li>electronic cassette automatically enters into data exchange mode - on the display of external panel <img class="srodek" src="rys_pc.jpg" width="50" height="18" border="0" alt="[rys_pc.jpg]" /> caption will be shown</li>
	<li>direct connection between EC electronic cassette and ISD-02 interface is possible</li>
</ul>

<p class="ret"><a href="#home">Back</a></p>	
</div>




<div class="ha2">
<h2><a name="wymianadanych">Exchange of data using MLX module</a></h2>
<p class="ret"><a href="#home">Back</a></p>	
</div>

<!-- ================================================================================================ -->
<div class="ha2">
<h2><a name="pamiecwewnetrzna">Internal memory</a></h2>
MLX module can be used as a portable memory module. It enables data exchange between electronic cassette and ISD-02 interface.
<p class="ret"><a href="#home">Back</a></p>	
</div>


<!-- ================================================================================================ -->
<div class="ha2">
<h2><a name="ecgolasko">EC - MLX connection</a></h2>
<table width="100%" cellspacing="5" cellpadding="5" border="0" class="tabelka">
<tr class="ciemny"><td><b>Newer type of electronic cassette - the connector is in the middle part of the PCB circuit</b></td></tr>
<tr><td><p><center><img src="ecmlx.jpg" width="739" height="355" border="0" alt="[ecmlx.jpg]" /></center></p></td></tr>
<tr class="ciemny"><td><b>Older type of electronic cassette - the connector is on the edge of the PCB circuit</b></td></tr>
<tr><td><p><center><img src="ecmlx2v2.jpg" width="739" height="355" border="0" alt="[ecmlx2v2.jpg]" /></center></p></td></tr>

</table>

<!--<p><center><img src="ecmlx.jpg" width="481" height="231" border="0" /></center></p>-->

<ul class="odstep">
	<li>connect MLX module to the socket in EC electronic cassette</li><br/>
	<p><b class="uwaga">NOTE!</b><br /> In case of an older type of electronic cassette the connection cable should be inserted only on the top row of pins.<br/>Coding inset in the plug should be at the top.<br/></p> 
	<li>on the display of external panel <img class="srodek" src="rys_ee.jpg" width="50" height="18" border="0" alt="" /> caption will be shown</li>
	<li>using keyboard in external panel one should choose appropriate option:</li>
	<ul class="odstep">
		<li><img class="srodek" src="rys_1.jpg" width="33" height="38" border="0" alt="" /> - backup data from electronic cassette to internal memory of MLX module - <img class="srodek" src="rys_bup.jpg" width="50" height="18" border="0" alt="" /></li>
		<li><img class="srodek" src="rys_2.jpg" width="33" height="38" border="0" alt="" /> - displays serial number of processor - <img class="srodek" src="rys_esn.jpg" width="50" height="18" border="0" alt="" /></li>
		<li><img class="srodek" src="rys_3.jpg" width="33" height="38" border="0" alt="" /> - upload data from MLX module to electronic cassette - <img class="srodek" src="rys_upl.jpg" width="50" height="18" border="0" alt="" /></li>
	</ul>
	<li>after selection the direction of data transfer (backup or upload) there are following options:</li>
	<ul class="odstep">
		<li><img class="srodek" src="rys_1.jpg" width="33" height="38" border="0" alt="" /> - copying all the parameters from the electronic cassette including database of identifiers - electronic keys - <img class="srodek" src="rys_all.jpg" width="50" height="18" border="0" alt="" /></li>
		<li><img class="srodek" src="rys_3.jpg" width="33" height="38" border="0" alt="" /> - copying only database of identifiers - electronic keys - <img class="srodek" src="rys_id.jpg" width="50" height="18" border="0" alt="" /></li>
	</ul>
	<li>the selection should be confirmed by touching on keyboard the field with the sign of key - writing or reading data to/from MLX module will began which is indicated by flashing 
	<img class="srodek" src="rys_bup.jpg" width="50" height="18" border="0" alt="" /> caption or adequately
	<img class="srodek" src="rys_upl.jpg" width="50" height="18" border="0" alt="" /></li>
	<li>after copying the data on the display <img class="srodek" src="rys_ee.jpg" width="50" height="18" border="0" alt="" /> caption will be shown and short acoustic signal will appear</li>
</ul>

<p class="ret"><a href="#home">Back</a></p>	
</div>



<!-- ================================================================================================ -->
<div class="ha2">
<h2><a name="n1">MLX - ISD-02 connection</a></h2>

<ul><li>Connect MLX module to the socket in ISD-02 interface</ul></li>
<p><center><img src="mlxisd.jpg" width="404" height="362" border="0" alt="[mlxisd.jpg]" /></center></p>

<p class="ret"><a href="#home">Back</a></p>	
</div>



<!-- ================================================================================================ -->
<div class="ha2">
<h2><a name="n2">DIP memory</a></h2>
<ul>
	<p><b class="uwaga">NOTE!</b><br /> <i>Applies only to electronic cassette equipped with memory chip in DIP package.</i></p>
	<li>remove U4 (24C64) memory chip from electronic cassette </li>
	<li>insert memory chip to the socket in MLX module</li>
	<li>connect MLX module to the socket in ISD-02 interface</li>
</ul>

<p class="ret"><a href="#home">Back</a></p>	
</div>



<!-- ================================================================================================ -->
<div class="ha2">
<h2><a name="n3">Receiving data from memory</a></h2>

<p>Since software version 6.7 of EC-2502 electronic cassette in DIP memory is stored a special identifier which identifies the type of entry phone system, software version of processor and operation mode of electronic cassette (U or H). It enables that during receiving data from memory, ISD-02 program identifies itself the kind of electronic cassette from which the data were collected.</p>
<p>In older versions of electronic cassettes those identifier does not exist and during first data receiving the program will ask what the kind of electronic cassette the data come from.</p>

<p class="fota"><img src="foto24.jpg" width="318" height="147" border="0" alt="[foto24.jpg]" /></p>

<p>One should choose from the list the appropriate type of electronic cassette.</p>

<p><b class="uwaga">NOTE!</b><br /> <i>Selection the type of electronic cassette and further saving the changes to memory will result also in identifier saving so one should be aware of choosing the right type.</i></p>

<p><b class="uwaga">NOTE!</b> <br /><i>Each time of receiving data from memory one should pay a special attention if ISD-02 program identify the type of electronic cassette correctly. In case of faulty reading one should set "<b>Data type ID</b>" parameter by itself.</i></p>

<p class="ret"><a href="#home">Back</a></p>	
</div>



<!-- ================================================================================================ -->
<div class="ha2">
<h2><a name="n4">Restoring default settings</a></h2>
<p class="fota"><img src="foto06.jpg" width="252" height="100" border="0" alt="[foto06.jpg]" /></p>
<p>Pressing "<b>Restore default values</b>" button will result in restore the default values of parameters only in specific branch.</p>

<p><b class="uwaga">NOTE!</b> <br /><i>It is possible to restore the default values <b>ONLY</b> for the parameters from P-1 and P-2 procedures.
Restore the default values of coded lock codes, individual settings, administrator password, serial number of processor and electronic cassette's data type ID is <b>IMPOSSIBLE</b>!</i>
</p>
<p>To restore the default values of coded lock codes and administrator password it is necessary to do this from electronic cassette's level.</p>

<p class="ret"><a href="#home">Back</a></p>	
</div>



<!-- ================================================================================================ -->
<div class="ha2">
<h2><a name="n5">Import/export data from/to file</a></h2>
<p>In ISD-02 program it is possible to import/export the following type of data from/to file:</p>
<ul>
	<li>all the parameters of electronic cassette including electronic keys database - support from "<b>PC</b>" panel; files with <b>*.bin</b> extension</li>
	<li>only coded lock codes and individual settings - files with <b>*.op</b> extension</li>
	<li>only identifiers - electronic keys database - files with <b>*.id</b> extension</li>
</ul>
<p>This easily allows to create a safety backup copies of settings of electronic cassette and restore lost settings in the future if necessary or e.g. by saving the electronic keys databases from few U electronic cassettes, use them in H electronic cassette which facilitate and quicken the configuration process of this electronic cassette.</p>

The files are located by default in <b>DATA</b> directory.

<p>An example of default file name is as follow <br/>
<center><b>2502_U65_1234_Dąbrowskiego 249.bin</b></center> <br/>
where:</p>

<table width="100%" cellspacing="5" cellpadding="5" border="0" class="tabelka">
<tr class="jasny"><td><b>2502</b></td><td>type of entry phone system CD-2502</td></tr>
<tr class="ciemny"><td><b>U65</b></td><td>operation mode U of electronic cassette, 6.5 software version of processor</td></tr>
<tr class="jasny"><td><b>1234</b></td><td>serial number stored in memory</td></tr>
<tr class="ciemny"><td><b>Dąbrowskiego 249</b></td><td>the value of "Object ID/Installation address" field</td></tr>

</table>

<p><b class="uwaga">NOTE!</b> <br /><i>It is recommended to create a safety backup copies in each edition of data!</i></p>

<p>Files with data saved on PC's hard disk can also be edited using text-editing software. </p>

<p class="ret"><a href="#home">Back</a></p>	
</div>



<!-- ================================================================================================ -->
<div class="ha2">
<h2><a name="n6">Export to *.op and *.id file</a></h2>
<ul>
	<li>In one of the tabs ("<b>Coded lock codes/Flats options</b>" or "<b>Identifiers - electronic keys</b>") select the area of rows to be saved. <br/><br/>
	<b class="uwaga">NOTE!</b> <br /><i>All the columns must be selected in the row/rows.<br /></i><br />
	To select the entire table use "<b>Ctrl+A</b>" key combination or select the title row using mouse.
	<li>right click on selected area or press "<b>Menu (application)</b>" key on the keyboard</li>
	<li>choose "<b>Save to file</b>" position</li>
	<li>save (press "<b>Save</b>" button) under suggested name or type your own one</li>
</ul>

<p class="fota"><img src="foto11.jpg" width="677" height="305" border="0" alt="[foto11.jpg]" /></p>
<p class="fota"><img src="foto20.jpg" width="283" height="124" border="0" alt="[foto20.jpg]" /></p>

<p class="ret"><a href="#home">Back</a></p>	
</div>



<!-- ================================================================================================ -->
<div class="ha2">
<h2><a name="n7">Import from *.op and *.id file</a></h2>

<ul>
	<li>select the cell in a row from which the data imported from file will be pasted</li>
	<li>right click on selected cell or press "<b>Menu (application)</b>" key on the keyboard</li>
	<li>choose "<b>Import from file</b>" position</li>
	<li>choose appropriate file from the list and press "<b>Open</b>" button</li>
</ul>

<p><b class="uwaga">NOTE!</b><br /> <i>Data that is imported from file will be inserted beginning from the row which cell is selected. Current data in the table will be replaced by imported data from file.</i></p>

<p><b>Example:</b><br /> If there were 12 numbers of electronic keys in the file, then while pasting them beginning from position 100, data that was placed on position from 100 to 111 will be removed and replaced with new one. </p>

<p class="fota"><img src="foto37.jpg" width="707" height="141" border="0" alt="[foto37.jpg]" /></p>
<p class="fota"><img src="foto33.jpg" width="228" height="145" border="0" alt="[foto33.jpg]" /></p>

<p class="ret"><a href="#home">Back</a></p>	
</div>






<!-- ================================================================================================ -->
<div class="ha2">
<h2><a name="n8">Copying/pasting data area</a></h2>

<p>In tabs "<b>Coded lock codes/Flats options</b>" and "<b>Identifiers - electronic keys</b>" there is a possibility to copy an area of data and paste it to another place. This allows to copy individual settings and sort of electronic keys database.</p>

<ul>
	<li>select the area of data to be copied<br /><br /><b class="uwaga">NOTE!</b><br /> <i>In case of "<b>Coded lock codes/Flats options</b>" tab,
	in selected area should not be present a cell/cells from "<b>Coded lock</b>" column. Further pasting of data will result in change of values of those cells for a new one.</i></li>
	<li style="list-style: none"><a name="home">&nbsp;</a></li>
	<li>right click on selected area or press "<b>Menu (application)</b>" key on the keyboard</li>
	<li>choose "<b>Copy</b>" position</li>
	<li>select the cell in a row from which the copied data will be pasted</li>
	<li>right click on selected cell or press "<b>Menu (application)</b>" key on the keyboard</li>
	<li>choose "<b>Paste</b>" position</li>
</ul>
<p><b class="uwaga">NOTE!</b><br /> <i>Pasted data will be inserted beginning from the row which cell is selected. Current data in the table will be replaced by imported data from file. Data will be replaced only in the cells from these columns which were previously copied.</i></p>

<p><b>Example:</b><br /> If there were 12 rows in copied area, then while pasting them beginning from position 100, data that was placed on position from 100 to 111 will be removed and replaced with new one. </p>

<p>It can be also used a combination of "<b>CTRL+C</b>" and "<b>CTRL+V</b>" keys to copy or paste the area of data.</p>
<p class="ret"><a href="#home">Back</a></p>	
</div>


<!-- ================================================================================================ -->
<div class="ha2">
<h2><a name="n9">Edition of electronic key</a></h2>

<p>ISD-02 interface allows to complete edition of identifiers - electronic keys (iButton and RFID) database with possibility of write/read it to/from file with *.id extension. Additionally keys can be easily moved to other positions and transferred from one electronic cassette to another which is useful e.g. during copying keys registered in few U electronic cassettes to H one.</p>

<p>Write/read to/from file the database of electronic keys - see "<b>Import/export data from/to file</b>" item.</p>

<p>Each application of electronic key to the ISD-02 interface results in displaying in fields "<b>Serial number ID</b>" and "<b>Serial number</b>" appropriate numbers.</p>

<p>In "<b>Destination of electronic keys - legend</b>" area are shown colors that match appropriate areas of electronic keys located in window of electronic keys database that are divided by type (destination).</p>

<p class="fota"><img src="foto07.jpg" width="354" height="310" border="0" alt="[foto07.jpg]" /></p>

<p class="ret"><a href="#home">Back</a></p>	
</div>

<!-- ================================================================================================ -->
<div class="ha2">
<h2><a name="dodawanietm">Addition of electronic key</a></h2>
<p class="ret"><a href="#home">Back</a></p>	
</div>


<!-- ================================================================================================ -->
<div class="ha2">
<h2><a name="a1">Addition of electronic key without assigned to the apartment</a></h2>

<ul>
	<li>press "<b>Add</b>" button</li>
	<li>put electronic key/keys against ISD-02 interface</li>
	<li>Electronic keys will be stored on the first available position. Position with added key will be highlighted.<br /><br/>
  <b class="uwaga">	NOTE! </b><br /><i>If applied key is already registered, it will be signaled by acoustic signal and by highlight the row where it is registered.</i></li>
</ul>
<p class="ret"><a href="#home">Back</a></p>	
</div>


<!-- ================================================================================================ -->
<div class="ha2">
<h2><a name="a2">Addition of electronic key with assigned to the apartment</a></h2>

<ul>
	<li>enter the number of apartment in "<b>Flat number</b>" field, which has to be assigned to the key/keys</li>
	<li>press "<b>Add to flat</b>" button</li>
	<li>put electronic key/keys against ISD-02 interface</li>
	<li>Electronic keys will be stored on the first available position. Position with added key will be highlighted. <br /><br/><b class="uwaga">NOTE!</b>
	<br /> <i>If applied key is already registered, it will be signaled by acoustic signal and by highlight the row where it is registered.</i></li>
</ul>

<p class="ret"><a href="#home">Back</a></p>	
</div>


<!-- ================================================================================================ -->
<div class="ha2">
<h2><a name="a3">Addition of electronic key on the selected item in memory</a></h2>


<ul>
	<li>choose a cell in "<b>ID No.</b>" column in a row where the key is going to be registered</li>
	<li>press "<b>Add to position</b>" button</li>
	<li>put electronic key against ISD-02 interface</li>
	<li>Electronic key will be stored on selected position and those position will be highlighted.<br /> <br/><b class="uwaga">NOTE!</b> <br /><i>If applied key is already registered, it will be signalled by acoustic signal and by highlight the row where it is registered.</i></li>
</ul>

<p class="ret"><a href="#home">Back</a></p>	
</div>


<!-- ================================================================================================ -->
<div class="ha2">
<h2><a name="a4">Searching for electronic key assigned to specific apartment</a></h2>

<ul>
	<li>in "<b>Searched flat number</b>" field enter the apartment number which keys assigned to it have to be searched</li>
	<li>press "<b>Find flat</b>" button</li>
	<li>if there are no keys assigned to this apartment then "<b>Position</b>" field will be grey</li>
	<li>if there are keys assigned to this apartment then positions on which they are registered will be displayed in "<b>Position</b>" field</li>
	<li>left click or pressing ENTER on the selected number in "<b>Position</b>" field results in selection of cell in "<b>ID No.</b>" column on selected position and highlighting the whole row. Edition of selected key is available.</li>
</ul>
<p class="ret"><a href="#home">Back</a></p>	
</div>


<!-- ================================================================================================ -->
<div class="ha2">
<h2><a name="a5">Checking for electronic key applied to ISD-02 interface</a></h2>

<p>There is a possibility to check if the key is already registered. To do this one should:</p>
<ul>
	<li>press "<b>Verify key</b>" button</li>
	<li>put electronic key/keys against ISD-02 interface</li>
	<li>If applied key is already registered, it will be signalled by acoustic signal and by highlight the row where it is registered.</li>
</ul>
<p class="ret"><a href="#home">Back</a></p>	
</div>


<!-- ================================================================================================ -->

<div class="ha2">
<h2><a name="a6">Changing electronic cassette operation mode</a></h2>
<p>In ISD-02 program there is possibility to change operation mode of electronic cassette <b>ONLY</b> from version U to H one. The operation in the opposite direction is impossible because of safety and confidentiality of coded lock codes. <br/>For the same reason it is not possible to restore the default values of coded lock codes.</p>
<p class="ret"><a href="#home">Back</a></p>	
</div>


<!-- ================================================================================================ -->
<div class="ha2">
<h2><a name="a7">Changing mode from U to H</a></h2>
<ul>
	<li>remember the values of parameters "<b>Serial number</b>" and "<b>Administrator password</b>"</li>
	<li>read binary file from <b>DATA\INIT_EC</b> directory that corresponds to the electronic cassette and the software version of the same types as the electronic cassette which has to be changed but in H version <br /><br/><b class="uwaga">NOTE!</b><br /> <i>Loaded binary file is equivalent to the default settings of electronic cassette for "<b>1234</b>" serial number</i></li>
	<li style="list-style: none"><a name="home">&nbsp;</a></li>
	<li>change the parameters "<b>Serial number</b>" and "<b>Administrator password</b>" to values previously remembered from U electronic cassette. <br/>In case the parameters "<b>Serial number</b>" and "<b>Administrator password</b>" have the same values that correspond to the processor serial number from electronic cassette, then such a configuration is equivalent to the situation after initialization (restoring the initial settings) of electronic cassette including erasing the whole database of electronic keys.</li>
</ul>
<p class="ret"><a href="#home">Back</a></p>	
</div>


<!-- ================================================================================================ -->
<div class="ha2">
<h2><a name="a8">Changing mode from H to U - requires support in external panel</a></h2>

<ul>
	<li>change the operation mode of electronic cassette from H to U in external panel</li>
	<li>make the initialization (restore the initial settings) of electronic cassette including erasing the whole database of electronic keys</li>
	<li>read the configuration from electronic cassette to the ISD-02 program</li>
</ul>

<p class="ret"><a href="#home">Back</a></p>	
</div>



<!-- ================================================================================================ -->
<div class="ha2">
<h2><a name="a9">Copying databases of electronic keys from few U electronic cassettes to H one</a></h2>

<ul>
	<li>in each of U electronic cassette write to *.id files the areas of electronic keys databases in which the keys are registered. <br /><br />
	<b class="uwaga">NOTE!</b><br /> <i> In case of fragmentary saving of electronic keys database it is recommended to save the different types of keys (normal, special and service) in separate files in order to its further easier discrimination and import.</i></li>
	<li style="list-style: none"><a name="home">&nbsp;</a></li>
	<li>import in turn previously saved files to H electronic cassette. <br /><br /><b class="uwaga">NOTE!</b><br /> <i>Pay attention that special and service keys from U electronic cassettes will be in the appropriate area of electronic keys database in H electronic cassette.</i></li>
</ul>

<p class="ret"><a href="#home">Back</a></p>	
</div>


</div>
</body>
</html>
