EC 3100 70U

# Parameters

-     Serial number

-     Administrator password

-     Data type identifier

-     Object Identifier/ Installation addresss

-     PIN code of external panel

-     [EtYP] - Operation mode of electronic cassette

-     [EnAu] - Sound signal of sign selected from the keyboard

-     [ tonY] - Multitone signalling of sign selected from the keyboard

-     [ tOc  ] - Waiting time for picking up the receiver

-     [  tro  ] - Time of conversation

-     [  t1t  ] - Time of individual tone generation

-     [ t1d  ] - Time of signal generation

-     [ tPA  ] - Pause time

-     [  F1   ] - Signal frequency F1

-     [  F2   ] - Signal frequency F2

-     [Sybr ] - Signalling number of the gate, from which a call has been received

-     [  trY  ] - Time of electrocatch operation

-     [ Ent  ] - 'Fast entrance'

-     [ CoEn] - Switching on coded lock service

-     [ CoEd] - Permission to edition of coded lock codes by occupants

-     [ CoPo] - Permission to confirm the use of lock code

-     [ CoEr] - Confirming the use of a wrong code of coded lock

-     [ ibEn] - Switching on/off electronic keys

-     [ ibAd] - Registration of electronic keys by users

-     [ nbL  ] - Block number

-->

-     [ Pnu  ] - Range shift

-     [ LPi   ] - Amount of rooms on the floor

-     [ LLo  ] - Range of serviced numbers ( low value)

-     [ LHi  ] - Range of serviced numbers ( high value)

-     [ LdP  ] - Directing of not serviced numbers

-     [ Ld1  ] - Additional number not included in the serviced range

# Lock codes / Locks Options

-     Physical number

-     Logical number

-     Lock code

-     Melody Nr.

-     Volume

-     Rings Nr.

-     Mode

-     Authorization

-     Lock code

# Electronic keys

-     Addition electronic key

-     Verification electronic key

-     Deleting electronic key

# Divided by subject

-     Numbering modes

-     Code of coded lock

-     Calling options

-     User blockade

-     Electronic keys

## Serial number

A unique serial number of the processor, according to which computes an array of electronics in the cassette lock codes. It is printed on a sticker on the processor.
You can edit it, which is useful for example in the case of edition operation mode of electronic cassette from U to H. It can take values from 0000 to 9999. If in the number is the digit 0, then it must also be entered.
Parameter changes can be made insection [ System parameters – grouped by functionality ].

top of page

## Administrator password

Default administrator password is the serial number printed on a sticker on the processor.
You can edit it in the ISD-02 program. It can take values from 0000 to 9999. If in the the number is the digit 0, then it must also be entered.
NOTE !
If you forget password, then without interface ISD-02 and ISD-02 program it is impossible to retrieve it and it will be necessary to restore the default settings of electronic cassette, which involves the loss of all entered settings.
Administrator password can be changed in section [ System parameters – grouped by functionality ].

top of page

## Data type identifier

Special identifier that identifies system type, software version and operation mode of electronic cassette ( U or H ). Data type identifier allow self identification of electronic cassette type during receiving data from the EEPROM memory to ISD-02 program.
NOTE !
During each process of receiving data from the EEPROM memory of it should be noted that the program correctly determined the electronic cassette type. In the case of an erroneous reading, set the parameter [Data type identifier] by yourself.

Data type identifier is composed of:

- first digit define operation mode of electronic cassette
  - 0 - subordinate entrance ( U ),
  - 1 – main entrance ( H ),
- next two digits identify the type of system
  - 52 – system CD-2502
  - 31 – system CD-3100
- last two digits indicate the version of the software –e.g. 65, 66, itp.

top of page

## Object Identifier / Installation addresss

addresss or name of the object, in which the electronic cassette is installed. Parameter help more easily identify files.
Name can contain 20 characters.
During saving data into files it will be default name of file -e.g.

3100_H70_1234_Dabrowskiego 249.bin
To change value [ Object Identifier/ Installation address] in section [ System parameters – grouped by functionality ].

top of page

## PIN code of external panel

Panels of doorphone systems CD-3100 are protected against theft by means of PIN codes. In order to use the panel, the PIN code supplied along with the panel by company Laskomex should be introduced only once.
Change is in section [ System parameters – grouped by functionality ].

top of page

## [ EtYP ] - Operation mode of electronic cassette

Parameter defining operation mode of electronic cassette:

- 0 - subordinate entrance - U
- 1 - main entrance - H

In a system with entrance hierarchy there are two types of entrances: the main entrance and subordinate entrances. System CD-3100 can operate for one main entrance and max. 64 subordinate entrances. From the main entrance a connection can be made with each apartment in any building or staircase serviced by the entry phone system. Using panels at the entrance to staircase (subordinate entrance) a connection can be made with the apartments located in this staircase only. Entry phones at subordinate entrances can be used independently. Default setting of the cassette is configured to operate with the subordinate entrance (U).

NOTE !
The parameter is not editable! To change the mode cassette electronics - see Menu/Instruction section Changing the Operation mode of electronic cassette.

top of page

## [ EnAu ] - Sound signal of sign selected from the keyboard

If this parameter is [ On ], then selection of any sign from the keyboard may be signalized with short acoustic signals heard on the speaker panel.

top of page

## [ tonY ] - Multitone signalling of sign selected from the keyboard

If this parameter is [ Off ], then selection of a key may be signalled with the same sound (one tone signalling) or (if [ tonY ]=[ On ]) for every key sound of different pitch may be attributed (multitone signalling). The use of this function requires fulfilling the following condition [ EnAu ]=1 and [ tonY ]=1.

top of page

## [ tOc ] - Waiting time for picking up the receiver

Parameter defines waiting time for receiver pick up in seconds after finishing of calling.

top of page

## [ tro ] - Time of conversation

Time of conversation between external panel user and uniphone user.
Conversation time after picking up the receiver is limited. 10 s before the lapse of conversation programmed time sound signals will be heard in the receiver, which will inform about approaching time of breaking.

top of page

## [ trY ] - Time of electrocatch operation

Time of electrocatch powering.

top of page

## [ Ent ] - 'Fast entrance'

Entry phone CD-2502 realizes functions "fast entrance" which is used only in entry phone with the main and subordinate entrances.
In entry phone without this function one must ring the occupant twice in order to get to his apartment (the first time at the main entrance and the second time at the entrance to the staircase). Function "fast entrance" eliminates the second step.

top of page

## [ CoEn ] - Switching on coded lock service

Setting parameter [ CoEn ] to [ Off ] value makes that function of coded lock will be switched off for all users regardless of setting for the individual apartments.
If parameter is set to [ On ] is possible switched off that function for indywidual users in section [ Lock codes / Locks Options ] setting parameter [ Lock code ] to "[-] - Off".

top of page

## [ CoEd ] - Permission to edition of coded lock codes by occupants

By default the occupants have the possibility to change the codes of a combination lock in user's menu. Setting this parameter to value [0] blocks this possibility to all occupants regardless of individual settings.
If parameter [ CoEd ] is [ On ] is possible to indywidual blocking edition of coded lock codes by occupants in section [ Lock codes / Locks Options ] by changing parameter [ Lock code ] to "[ E ] - Act.+Edition".
NOTE !
Edition by user is possible ONLY in subordinate entrance ( U ).

top of page

## [ CoPo ] - Permission to confirm the use of lock code

Each unblocking of door by means of a coded lock makes that three short acoustic signals are generated in a uniphone mounted in an apartment whose code was used to open the door.
Parameter set to [0] enables to switch off this signalization in all uniphones. The Signalling can be switched off for the selected numbers.

top of page

## [ CoEr ] - Confirming the use of a wrong code of coded lock

Entering the wrong code to a combination lock makes that two long acoustic signals will be generated in a uniphone mounted in an apartment to which there was an attempt to use a code to open the door. This is a signal for occupants that somebody tries to break the code of a combination lock.
This option ([ CoEr ]=[ Off ])allows switching off this signalization in all uniphones.

top of page

## [ ibEn ] - Switching on/off electronic keys

In section [ System parameters – grouped by functionality → Code lock parameters] or [ Parameters – order according to the system → Bit Parameters ] default value parameter [ ibEn ] is [ On ] - function of coded lock is switched on for all users.

top of page

## [ ibAd ] - Registration of electronic keys by users

In a system is possible registration of electronic keys by users. Setting parameter [ ibAd ] value to [ On ] in section [ System parameters – grouped by functionality → Code lock parameters] or [ Parameters – order according to the system → Bit Parameters ] permits users to register new electronic keys from user's menu.

top of page

## [ nbL ] - Mode with building numbering

Switches on the mode with the building numbering. This numbering mode can be used only in entry phone system with entrance hierarchy (main entrance and subordinate entrances). This numbering mode allows repeating apartment numbers in different buildings.
In electronic cassette for subordinate entrance set parameter [ nbL ] (block number) to value higher then zero.
The operation should be repeated for other staircases (buildings). Values [ nbL ] can be repeated in subordinate systems provided that these systems operate with other logical numbers of uniphones.
In order to get connection with an apartment from an external panel at the main entrance one should first of all select building number and then apartment number.

In electronic cassette for main entrance set parameter [ NrbL ] to value [ On ].

top of page

## [ Pnu ] - Range shift

Setting parameter [ Pnu ] to value higher then 0 switching on numbering mode with range shift.
In this numbering mode physical number of a uniphone (programmed by jumpers) differs from its logical number (under which a uniphone rings after having selected the number from the keyboard).
This numbering mode is used for apartments of numbers higher than 255.

logical number = physical number + range shift
Example:
In a building an entry phone should be used for apartments Nos. 301...310.
In uniphones physical numbers should be programmed as follows: in apartment 301 number 1, in apartment 302 number 2 etc.
Then parameter of range shift [ Pnu ] should be set to value 300.
After having done this and selecting from a keyboard number 301 the uniphone in which number 1 has been programmed will ring, after having selected number 302 uniphone with number 2 will ring etc.

top of page

## [ LPi ] - Amount of rooms on the floor

Setting parameter [ LPi ] to value higher then 0 switching on hotel numbering mode.
This numbering mode is meant for the buildings in which room number starts with a digit defining number of floor on which the room is located (hotels, resort houses, dormitories etc.).
Physical number of a uniphone is calculated according to the formula:

Physical number = P * LL + XX
where
P - floor number,
LL - amount of rooms on one floor (value of parameter [ LPi ])
XX - number of room on the floor ( number from the range 1 ... [ LPi ])

top of page

## [ LLo ] - Range of serviced numbers ( low value)

Parameter is used to set number range which is serviced by an entry phone. After selecting a number outside this range a message will appear on the display [ OFF ].
Limiting the range is recommended especially in case of an entry phone in a multi-entrance version.
Be careful that [ LLo ] < [ LHi ]. Otherwise selecting of any number will result in displaying a message [ OFF ].

top of page

## [ LHi ] - Range of serviced numbers ( high value)

Parameter is used to set number range which is serviced by an entry phone. After selecting a number outside this range a message will appear on the display [ OFF ].
Limiting the range is recommended especially in case of an entry phone in a multi-entrance version.
Be careful that [ LLo ] < [ LHi ]. Otherwise selecting of any number will result in displaying a message [ OFF ].

top of page

## [ LdP ] - Directing of not serviced numbers

All numbers which are not serviced by entry phone CD-3100, will be directed to uniphone number given as [ LdP ] value

top of page

## [ Ld1 ] - Additional number not included in the serviced range

In many cases it is necessary to operate numbers which do not belong to the operated range.
For each of numbers [ Ld1 ],[ Ld2 ], [ Ld3 ] and [ Ld4 ] it is possible to set individually any number from the range 1...9998.

top of page

# Divided by subject

## Numbering modes

Digital entry phone as a standard can operate numbers within a range 1...255 (Normal mode), however, very often it is necessary to operate higher numbers or numbers of considerably wider range. This is possible owing to different numbering modes:

- Numbering mode with range shift
- Hotel numbering mode
- Mode with building numbering

### Physical number

Number of uniphone (programmed by jumpers) within a range 1...255.

### Logical number

Number under which a uniphone rings after having selected the number from the keyboard - within a range 1...9998.

### Normal mode

In normal mode physical number of uniphone (programmed by jumpers) corresponds to logical number (selected from the keyboard of talking cassette). This is a default mode of operation of entry phone exchange.

### Numbering mode with range shift

In this numbering mode physical number of a uniphone (programmed by jumpers) differs from its logical number (under which a uniphone rings after having selected the number from the keyboard).
This numbering mode is used for apartments of numbers higher than 255.
Physical number of a uniphone is calculated according to the formula:

logical number = physical number + range shift
This numbering mode is switched on in a moment of setting of parameter [ Pnu ] to the value higher than [0].
Example:
In a building an entry phone should be used for apartments Nos. 301...310.
In uniphones physical numbers should be programmed as follows: in apartment 301 number 1, in apartment 302 number 2 etc.
Then parameter of range shift [ Pnu ] should be set to value 300.
After having done this and selecting from a keyboard number 301 the uniphone in which number 1 has been programmed will ring, after having selected number 302 uniphone with number 2 will ring etc.

### Hotel numbering mode

This numbering mode is meant for the buildings in which room number starts with a digit defining number of floor on which the room is located (hotels, resort houses, dormitories etc.).
Physical number of a uniphone is calculated according to the formula:

Physical number = P * LL + XX
where
P - floor number,
LL - amount of rooms on one floor (value of parameter [ LPi ])
XX - number of room on the floor, number from the range (1 ... [ LPi ])

This numbering mode will be activated at the moment of setting the value of parameter [ LPi ] to value higher than zero.

### Mode with building numbering

This numbering mode can be used only in entry phone system with entrance hierarchy. This numbering mode allows repeating apartment numbers in different buildings.
In order to get connection with an apartment from an external panel at the main entrance one should first of all select building number and then apartment number.
In electronic cassette for subordinate entrance set parameter [ nbL ] (block number) to value higher then zero and in electronic cassette for main entrance parameter [ NrbL ] to value [ On ].
Values [ nbL ] can be repeated in subordinate systems provided that these systems operate with other logical numbers of uniphones.

### Additional numbers

In many cases it is necessary to operate numbers which do not belong to the operated range.
For each of numbers [ Ld1 ],[ Ld2 ], [ Ld3 ] and [ Ld4 ] it is possible to set individually any number from the range 1...9998.

### Range of operated numbers(logical)

- [ LLo ] - Range of serviced numbers ( low value) - Physical number representing the low value of the range.
- [ LHi ] - Range of serviced numbers ( high value) - Physical number representing the high value of the range.

In default setting the operation of all apartment numbers is included. If the range is limited (parameters [ LLo ] and [LHi ] ), selection of a number outside the set range will result in displayed message [ OFF ].
Be careful that[ LLo ] < [ LHi ]. Otherwise selecting of any number will result in displaying a message [ OFF ]. Limiting is set for physical not logical numbers!
Default set range 1...250.

### Directing of not serviced numbers

All numbers which are not serviced by entry phone, will be directed to uniphone number given as [ LdP ] value

top of page

## Code of coded lock

To each apartment one four digital number is attributed which is preliminary defined in the entry phone production process.
To activate this function set parameter [ CoEn ] to [ On ]. Function of coded lock will be switched on for all users regardless of setting for the individual apartments.
Code of coded lock can be changed by installing specialist or user (if parameter [ CoEd ] is set to [ On ]).
Code of coded lock are declared only in the subordinate entrance cassette (U).

### Confirming the use of code of coded lock

Each unblocking of door by means of a coded lock ( correctly or wrongly) makes that acoustic signals are generated in a uniphone mounted in an apartment whose code was used to open the door.

- [ CoPo] - Confirming the use of correctly code of coded lock - three short acoustic signals
- [ CoEr] - Confirming the use of wrongly code of coded lock - two long acoustic signals

Parameter set to [0] enables to switch off this signalization in all uniphones.

### changing the code of coded lock

In section [ Lock codes / Locks Options ] can be change codes of coded lock for individual users.
NOTE !
In the interests of the existing electronic cassettes the program does not allow to restore the default codes of coded lock.
It would be enable to generate the correct code of coded lock by any other person. Therefore, restoring the default code of coded lock is only possible from the configuration procedures in electronic cassette.

### Special cods

There isn't special cods dedicated for postmen, administration. Special codes can be attributed to one of additional numbers: [ Ld1 ], [ Ld2 ], [ Ld3 ] , [ Ld4 ] or to number witch isn't use by anyone.

### Individual settings - edition by users

Parameter [Lock code] - Options of combination lock for indywidual users:

- "[ - ] - Off" - Combination lock switched off
- [ A ] - Active - Combination lock activated, occupant can neither change the code or register electronic keys
- [ E ] - Act. + Edition - Combination lock activated, occupant may change the code and register electronic keys

in section [ Lock codes / Locks Options ].

top of page

## Calling options

Calling signal consists of several parts:

- Calling signal – multiplicity of parameters:
  - Time of individual tone generation [ t1t ] - consists of three tones of different frequency F0 (1 kHz), F1 and F2
  - Time of signal generation [ t1d ]
  - Pause time between successive signals ( if number of bells are set to more then 1) [ tPA ]
  and
- Waiting time for picking up the receiver [ tOC ]

Parameters: number of bells, calling ton, calling volume can be set for indywidual users. Signal frequency, time of individual tone generation, pause time, waiting time for picking up the receiver are global parameters for all users conected to this electronic cassette.

### [ t1t ]

Time of individual tone generation [*10ms]
Successive tons of different frequency [ F0 ] (1 kHz), [ F1 ] and [ F2 ] form single signal [ t1d ].

### [ t1d ]

Time of signal generation [*10ms] consists of signals [ t1t ] of different frequency.

### [ tPA ]

Pause time *10[ms] after signal [ t1d ]

### [ F1 ]

Signal frequency F1 [*10Hz]

### [ F2 ]

Signal frequency F2 [*10Hz]

### [ tOc ]

Waiting time for picking up the receiver in seconds

### [Sybr]

Signalling number of the gate, from which a call has been received.
When a call from slave entrance is being received, the doorphone may signal acoustically entrance number, from which such a call is coming from. The number is signalized with a short acoustic signal after each calling cycle.

### Melody Nr.

Parameter can take values from the range 0...7. Parameter value is defined by one of 8 pre-defined calling tones.

### Volume

Entry phone enables setting three volume levels and calling of increasing volume (requires setting at least two bells):

- [C] - silent bell
- [U] - moderate bell
- [G] - loud bell
- [N] - increasing bell.

### Rings Nr.

Parameter can take values from the range 0...7.

top of page

## Authorization

In the entry phone it is possible to define how the pushbutton operates the electro-catch at the individual entrances:

- [-] - blockade - No electro-catch control from the uniphone (monitor)
- [U] - only U - Pushbutton activates electro-catch at the subordinate entrance only
- [H] - only H - Pushbutton activates electro-catch at the main entrance only
- [A] - U+H - Pushbutton activates electro-catch at the main entrance and at the subordinate entrance

top of page

## User blockade

It is possible to limit possibility of opening entrances, possibility of talking or blocking the uniphone.

### possibility of opening entrances

Switching off possibility of opening entrances - setting parameter [Authorization] in section [ Lock codes / Locks Options ] to "[ - ] - Off".
It is possible to limit selectively possibility of opening entrances (U orH):

- [A] - Pushbutton activates electro-catch at the main entrance and at the subordinate entrance [ U + H ],
- [H] - Pushbutton activates electro-catch at the main entrance only ,
- [U] - Pushbutton activates electro-catch at the subordinate entrance only

NOTE !
User can change parameter in USER'S MENU

### Blocking possibility of talking (uniphone functions as a bell)

Uniphone may be called, however, conversation cannot be conducted and electro-catch cannot be controlled. Blockade will be activated after changing parameter [Mode] in section [ Lock codes / Locks Options ] to "[d]- Bell".
NOTE !
User can change parameter in USER'S MENU

### Uniphone blockade

Uniphone switched off. Changing parameter [Mode] in section [ Lock codes / Locks Options ] to "[ - ] - Off" makes that it is impossible to make a connection with the apartment for which such setting was selected. An attempt to make a connection will be followed by a message [ OFF ] .
NOTE !
User can not change parameter in USER'S MENU

top of page

## [Mode]

If needed entry phone reaction after calling can be changed:

- [ - ]- Off - Uniphone switched off
- [ d ]- Bell - Blocking possibility of talking (uniphone functions as a bell)
- [ A ]- Active - Active uniphone

Parameter [Mode] can be changed in section [ Lock codes / Locks Options ].

top of page

## Electronic keys

Entry phone CD-3100 can be equipped with electronic key reader. There are three kinds of keys in entry phone:

- service keys enable change of entry phone configuration,
- special keys are used by postmen, administration etc.
- keys for the occupants.

Keys should be registered at both the main and subordinate entrance. At the main entrance keys attributed to apartment cannot be registered. Entry phone users can register their own electronic keys. This possibility can be switched on globally by setting parameter [ ibAd] to value [ On ].

- Switching on electronic key
  Default value parameter [ ibEn] is [ On ] - users can register their own electronic keys. In another case, parameter [ ibEn] should be changed in main and subordinate entrance electronic cassette.
- Registration of electronic keys by users
  In a system is possible registration of electronic keys by users. Setting parameter [ ibAd ] value to [ On ]

### Addition

ISD-02 interface allow registration electronic keys in electronic cassette, addition of keys with attributing to apartment, addition on the selected item in memory, and copying keys ( all or whole section) from one electronic cassette to other, or saving settings in file. Using program ISD-02 it is possible to write and read data to the table to / from a file with the extension *.tm, that is so after programmed keys in one electronic cassette it is easily to copy it to another located in the system (for example, to copy from subordinate entrance cassette tapes to main entrance cassette). To save the table select in section [ Electronic keys ] the area you want to copy and press the right mouse button and choose [ Save to file ], and give it a name. To load data into an table, press the right mouse button in the line of the table and choose [ Import from file ].
NOTE !
The data that we import from the file will be inserted into the cell line which pointed out. Data in the table will be replaced data imported from the file.
Example:
In file is 12 keys, if we paste them from position 100 then data from positions 100-111 will be deleted and replaced by new. Saved file can be edited. To make change it should be opened in any program to text edition (eg. notepad) made data changes, and finally file must be saved
Besides addition keys by installing specialist it is possible addition keys by users after setting parameter [ ibAd] to [ On ].

The program allows addition:

#### One electronic key

If you want to add one electronic key, then in section [ Electronic keys ] choose [ Add ] and apply key to the reader ISD. The serial number of electronic key will bereading and show in the box [Serial Number]. This key will be add to first free position. If this key was earlier registrated it will not be add – line with this particular key will be highlighted.

#### Several keys at once

If you want to add several keys at once, then choose [ Add ] and apply all keys successively to the reader ISD. They will be successively added to the first free position.

#### Addition to Flat

If you want to add one electronic key to particular flat, then in section [ Electronic keys ] choose [ Add to Flat ], write number of this flat and apply key to the reader ISD. Electronic key will be add to first free position.

#### Addition to Position

If you want to add one electronic key to particular position, then in section [ Electronic keys ]:

- select the position of the cursor,
- choose [ Add to Position ]
- apply key to the reader ISD.

### Verification

#### Verification the key is already registered in the system

If you want to verify that the key is already registered in the system - in section [ Electronic keys ] choose [ Verify key ] and apply key to the reader ISD. If this key was earlier registrated line with this particular key will be highlighted.

#### Verification the key is already registered in the flat

If you want to verify that the key is already registered in specific flat - write number of this flat and choose [ Find flat ]. In box [ Position ] will be specify numbers of positions where is this number of flat. After mark this position and double pressing of left button on mouse line with this particular flat will be highlighted.

### Registering one key in several electronic cassettes

There is possibility of addition one key to several electronic cassette (eg. several subordinate entrances and one main entrance, or only to subordinate entrances). For postmen, administration etc. aside an area designated numbers 1000-1019, which can select and save the file, and during programming other electronic cassette import selected area table to area designed for special keys used by postmen, administration etc. in section [ Electronic keys ].

### Deleting key

Deleting the key from memory will take place after marking line with key and pressing on the keyboard 'Delete'. Deleting all keys from memory will take place after marking any cell in the table and pressing at the same time 'ctrl' and 'a'on the keyboard and next 'Delete'.

top of page

###### v1.0 (24-11-2010)